

Consumer Confidence Report	Page 5 of 9
[bookmark: _Toc58336712]2025 Consumer Confidence Report
[bookmark: _Toc58336713]Water System Information
Water System Name: 1910138 – Los Angeles World Airports
Report Date: June 29, 2026
Type of Water Source(s) in Use: Groundwater
Name and General Location of Source(s): East and West Wells located at 2825 E. Avenue P, Palmdale, CA 93550
Drinking Water Source Assessment Information: [Enter Drinking Water Source Assessment Information]
Time and Place of Regularly Scheduled Board Meetings for Public Participation: [Enter Time and Place of Regularly Scheduled Board Meetings for Public Participation]
For More Information, Contact: [Enter Water System’s Contact Name and Phone Number]
[bookmark: _Toc58336714]About This Report
We test the drinking water quality for many constituents as required by state and federal regulations.  This report shows the results of our monitoring for the period of January 1 to December 31, 2025, and may include earlier monitoring data.
Importance of This Report Statement in Five Non-English Languages (Spanish, Mandarin, Tagalog, Vietnamese, and Hmong)
Language in Spanish:  Este informe contiene información muy importante sobre su agua para beber.  Favor de comunicarse [Enter Water System’s Name] a [Enter Water System’s Address or Phone Number] para asistirlo en español.
Language in Mandarin:  这份报告含有关于您的饮用水的重要讯息。请用以下地址和电话联系 [Enter Water System Name]以获得中文的帮助: [Enter Water System’s Address][Enter Water System’s Phone Number].
Language in Tagalog: Ang pag-uulat na ito ay naglalaman ng mahalagang impormasyon tungkol sa inyong inuming tubig.  Mangyaring makipag-ugnayan sa [Enter Water System’s Name and Address] o tumawag sa [Enter Water System’s Phone Number] para matulungan sa wikang Tagalog.
Language in Vietnamese:  Báo cáo này chứa thông tin quan trọng về nước uống của bạn.  Xin vui lòng liên hệ [Enter Water System’s Name] tại [Enter Water System’s Address or Phone Number] để được hỗ trợ giúp bằng tiếng Việt.
Language in Hmong:  Tsab ntawv no muaj cov ntsiab lus tseem ceeb txog koj cov dej haus.  Thov hu rau [Enter Water System’s Name] ntawm [Enter Water System’s Address or Phone Number ] rau kev pab hauv lus Askiv.
[bookmark: _Toc58336715]Terms Used in This Report
	Term
	Definition

	Level 1 Assessment
	A Level 1 assessment is a study of the water system to identify potential problems and determine (if possible) why total coliform bacteria have been found in our water system.

	Level 2 Assessment
	A Level 2 assessment is a very detailed study of the water system to identify potential problems and determine (if possible) why an E. coli MCL violation has occurred and/or why total coliform bacteria have been found in our water system on multiple occasions.

	Maximum Contaminant Level (MCL)
	The highest level of a contaminant that is allowed in drinking water.  Primary MCLs are set as close to the PHGs (or MCLGs) as is economically and technologically feasible.  Secondary MCLs are set to protect the odor, taste, and appearance of drinking water.

	Maximum Contaminant Level Goal (MCLG)
	The level of a contaminant in drinking water below which there is no known or expected risk to health.  MCLGs are set by the U.S. Environmental Protection Agency (U.S. EPA).

	Maximum Residual Disinfectant Level (MRDL)
	The highest level of a disinfectant allowed in drinking water.  There is convincing evidence that addition of a disinfectant is necessary for control of microbial contaminants.

	Maximum Residual Disinfectant Level Goal (MRDLG)
	The level of a drinking water disinfectant below which there is no known or expected risk to health.  MRDLGs do not reflect the benefits of the use of disinfectants to control microbial contaminants.

	Primary Drinking Water Standards (PDWS)
	MCLs and MRDLs for contaminants that affect health along with their monitoring and reporting requirements, and water treatment requirements.

	Public Health Goal
(PHG)
	The level of a contaminant in drinking water below which there is no known or expected risk to health.  PHGs are set by the California Environmental Protection Agency.

	Regulatory Action Level
(AL)
	The concentration of a contaminant which, if exceeded, triggers treatment or other requirements that a water system must follow.

	Secondary Drinking Water Standards (SDWS)
	MCLs for contaminants that affect taste, odor, or appearance of the drinking water.  Contaminants with SDWSs do not affect the health at the MCL levels.

	Treatment Technique
(TT)
	A required process intended to reduce the level of a contaminant in drinking water.

	Variances and Exemptions
	Permissions from the State Water Resources Control Board (State Board) to exceed an MCL or not comply with a treatment technique under certain conditions.

	ND
	Not detectable at testing limit.

	ppm
	parts per million or milligrams per liter (mg/L)

	ppb
	parts per billion or micrograms per liter (µg/L)

	ppt
	parts per trillion or nanograms per liter (ng/L)

	ppq
	parts per quadrillion or picogram per liter (pg/L)

	pCi/L
	picocuries per liter (a measure of radiation)


[bookmark: _Toc58336716]Sources of Drinking Water and Contaminants that May Be Present in Source Water
The sources of drinking water (both tap water and bottled water) include rivers, lakes, streams, ponds, reservoirs, springs, and wells.  As water travels over the surface of the land or through the ground, it dissolves naturally-occurring minerals and, in some cases, radioactive material, and can pick up substances resulting from the presence of animals or from human activity.
Contaminants that may be present in source water include:
Microbial contaminants, such as viruses and bacteria, that may come from sewage treatment plants, septic systems, agricultural livestock operations, and wildlife.
Inorganic contaminants, such as salts and metals, that can be naturally-occurring or result from urban stormwater runoff, industrial or domestic wastewater discharges, oil and gas production, mining, or farming.
Pesticides and herbicides, that may come from a variety of sources such as agriculture, urban stormwater runoff, and residential uses.
Organic chemical contaminants, including synthetic and volatile organic chemicals, that are byproducts of industrial processes and petroleum production, and can also come from gas stations, urban stormwater runoff, agricultural application, and septic systems.
Radioactive contaminants, that can be naturally-occurring or be the result of oil and gas production and mining activities.
Regulation of Drinking Water and Bottled Water Quality
In order to ensure that tap water is safe to drink, the U.S. EPA and the State Board prescribe regulations that limit the amount of certain contaminants in water provided by public water systems.  The U.S. Food and Drug Administration regulations and California law also establish limits for contaminants in bottled water that provide the same protection for public health.
[bookmark: _Toc58336717]About Your Drinking Water Quality
[bookmark: _Toc58336718][bookmark: _Hlk57994699]Drinking Water Contaminants Detected
Tables 1, 2, 3, 4, 5, 6, and 8 list all of the drinking water contaminants that were detected during the most recent sampling for the constituent.  The presence of these contaminants in the water does not necessarily indicate that the water poses a health risk.  The State Board allows us to monitor for certain contaminants less than once per year because the concentrations of these contaminants do not change frequently.  Some of the data, though representative of the water quality, are more than one year old.  Any violation of an AL, MCL, MRDL, or TT is asterisked.  Additional information regarding the violation is provided later in this report.
Table 1.  Sampling Results Showing the Detection of Coliform Bacteria
Complete if bacteria are detected.

	Microbiological Contaminants 
	Highest No. of Detections
	No. of Months in Violation
	MCL
	MCLG
	Typical Source of Bacteria

	E. coli

	0
	0
	(a)
	0
	Human and animal fecal waste

	Total coliform
	0
	0
	(a)
	None
	Naturally occurring in the environment



(a) Routine and repeat samples are total coliform-positive and either is E. coli-positive or system fails to take repeat samples following E. coli-positive routine sample or system fails to analyze total coliform-positive repeat sample for E. coli.
Table 2.  Sampling Results Showing the Detection of Lead and Copper
Complete if lead or copper is detected in the last sample set.

	Lead and Copper 
	Sample Date
	No. of Samples Collected
	90th Percentile Level Detected
	No. Sites Exceeding AL
	Range of Results
	AL
	PHG
	Typical Source of
Contaminant

	Lead (ppb)
	August 2024
	10
	0.0
	N/A
	0 – 0
]
	15
	0.2
	Corrosion of household plumbing systems; Erosion of natural deposits

	Copper (ppm)
	August 2024
	10
	0.0
	N/A
	0 – 0

	1.3
	0.3
	Internal corrosion of household plumbing systems; erosion of natural deposits; leaching from wood preservatives



Los Angeles World Airports Palmdale has completed the initial lead service line inventory required by U.S. EPA’s Lead and Copper Rule Revisions. The deadline for the initial inventories was October 16, 2024.
Through completing a historical records review and field investigations, Los Angeles World Airports Palmdale has determined it has no lead or galvanized requiring replacement service lines in its distribution system.
Los Angeles World Airports Palmdale reviewed all applicable sources of information, including:
· All construction and plumbing codes, permits, and existing records or other documentation that indicates the service line materials;
· All water system records, including distribution system maps and drawings, historical records on each service connection, and standard operating procedures;
· All previous service line or meter replacements were conducted.
In addition to reviewing the above sources of information, Los Angeles World Airports Palmdale physically inspected all service lines in its distribution system, regardless of ownership. All service lines were verified non-lead.
Los Angeles World Airports Palmdale will update service line material information obtained from normal operations, such as service line maintenance, installation, or water meter readings, after October 2024 and will update the initial inventory accordingly.

Table 3.  Sampling Results for Sodium and Hardness
	Chemical or Constituent (and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
	PHG (MCLG)
	Typical Source of Contaminant

	Sodium (ppm)
	2/2/2023
	36
	30-36
	None
	None
	Salt present in the water and is generally naturally occurring

	Hardness (ppm)
	2/2/2023
	70
	58-70
	None
	None
	Sum of polyvalent cations present in the water, generally magnesium and calcium, and are usually naturally occurring


Table 4.  Detection of Contaminants with a Primary Drinking Water Standard
	Chemical or Constituent
(and
reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL [MRDL]
	PHG (MCLG) [MRDLG]
	Typical Source of Contaminant

	Antimony (ug/L)
	2/2/23
	<2
	N/A
	6
	6
	Discharge from petroleum refineries; fire retardants; ceramics; electronics; solder

	Arsenic (ug/L)
	2/2/23
	<2
	N/A
	10
	0
	Erosion of natural deposits; runoff from orchards, runoff from glass and electronics production wastes

	Barium (ug/L) 
	2/2/23 
	24 
	19-24
	2000 
	2000 
	Discharge of oil drilling wastes and from metal refineries; erosion of natural deposits 

	Beryllium (ug/L)
	2/2/23
	<1
	N/A
	4
	4
	Discharge from metal refineries and coal-burning factories; discharge from electrical, aerospace, and defense industries

	Cadmium (ug/L) 
	2/2/23 
	<1 
	N/A 
	5 
	5 
	Corrosion of galvanized pipes; erosion of natural deposits; discharge from metal refineries; runoff from waste batteries and paints 

	Chromium (ug/L) 
	2/2/23 
	<10
	N/A 
	100 
	100 
	Erosion of natural deposits 

	Cyanide (ug/L) 
	07/14/25 
	<5 
	N/A 
	200 
	200 
	Discharge from steel/metal factories, plastic and fertilizer factories 

	1,2-dichloroethane (ug/L) 
	07/14/25 
	<0.5 
	N/A 
	5
	0
	Discharge from industrial chemical factories  

	Cis-1,2-dichloroethylene (ug/L) 
	07/14/25 
	<0.5 
	N/A 
	70 
	70 
	Discharge from industrial chemical factories  

	trans-1,2-Dichloroethylene (ug/L) 
	07/14/25 
	<0.5 
	N/A 
	100 
	100 
	Discharge from industrial chemical factories  

	1,2-Dichloropropane (ug/L) 
	07/14/25 
	<0.5 
	N/A 
	5 
	0 
	Discharge from industrial chemical factories  

	Ethylbenzene (ug/L) 
	07/14/25 
	<0.5 
	N/A 
	700 
	700 
	Discharge from petroleum refineries 

	Fluoride (mg/L) 
	2/2/23 
	0.085
	0.055-0.085 
	4 
	4 
	Water additive which promotes strong teeth; erosion of natural deposits; discharge from fertilizer and aluminum factories 

	Mercury (ug/L) 
	8/19/24 
	<0.2 
	N/A 
	2 
	2 
	Erosion of natural deposits; discharge from refineries and factories; runoff from landfills and croplands 

	Nitrate (mg/L) 
	07/14/25
	0.85 
	0.52-0.68 
	10 
	10 
	Runoff from fertilizer use; leaching from septic tanks, sewage; erosion of natural deposits 

	Nitrite (mg/L) 
	07/14/25
	<0.05 
	N/A 
	1 
	1 
	Runoff from fertilizer use; leaching from septic tanks, sewage; erosion of natural deposits 

	Radium-226 (PCI/L) 
	9/2/22 
	<0.375 
	N/A 
	       5
	0 
	Erosion of natural deposits 

	Selenium (ug/L) 
	2/2/23 
	<2 
	N/A 
	50 
	50 
	Discharge from petroleum and metal refineries; erosion of natural deposits; discharge from mines 

	Tetrachloroethylene (ug/L) 
	07/14/25 
	<0.5 
	N/A 
	5 
	0 
	Discharge from factories and dry cleaners 

	Thallium (ug/L) 
	2/2/23 
	<1 
	N/A 
	2 
	0.5 
	Leaching from ore-processing sites; discharge from electronics, glass, and drug factories 

	Toluene (ug/L) 
	07/14/25
	<0.5 
	N/A 
	1000 
	1000 
	Discharge from petroleum factories 

	1,2,4- Trichlorobenzene (ug/L) 
	07/14/25
	<0.5 
	N/A 
	70 
	70 
	Discharge from textile finishing factories 

	1,1,1- Trichloroethane (ug/L) 
	07/14/25
	<0.5 
	N/A 
	2000 
	200 
	Discharge from metal degreasing sites and other factories 

	1,1,2- Trichloroethane (ug/L) 
	07/14/25
	<0.5 
	N/A 
	5 
	3 
	Discharge from industrial chemical factories 


Table 5.  Detection of Contaminants with a Secondary Drinking Water Standard
	Chemical or Constituent (and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	SMCL
	PHG (MCLG)
	Typical Source
of
Contaminant

	Aluminum (ug/L)
	2/2/23
	170
	<50-170
	50-200
	None
	deposits; residual from some surface water treatment processes

	Chloride (mg/L)
	2/2/23 
	9.4
	9.2-9.4
	250
	None
	Salt present in the water and is generally naturally occurring

	Color (color units)
	1/13/25
10/5/23
	1.0
	1.0-1.0
	15
	None
	Naturally-occurring organic materials

	Odor (odor units)
	1/13/25
10/5/23
	4.0
	<1.0-4.0 
	3
	None
	Naturally occurring organic materials

	Iron (ug/L)
	2/2/23
	340
	<50-340
	300
	None
	Iron-bearing soil and rock

	pH
	2/2/23
	8.32
	8.21-8.32
	6.5-8.5
	None
	Naturally occurring organic materials

	Sulfate (mg/L)
	2/2/23
	20
	17-20
	250
	None
	Mineral dissolution, atmospheric deposition, mining, fertilizer

	Total Dissolved Solids [TDS] (mg/L)
	2/2/23
	180
	160-180
	500
	None
	Generally naturally occurring 

	Turbidity (NTU)
	1/13/25
10/5/23
	1.1
	< 0.1 – 1.1
	5
	None
	Soil runoff

	Zinc (ug/L)
	12/2/25
	<50
	N/A
	5000
	None
	Naturally occurring organic materials


Table 6.  Detection of Unregulated Contaminants
	Chemical or Constituent (and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	Notification Level
	Health Effects 

	None
	N/A
	N/A
	N/A
	N/A
	N/A


[bookmark: _Toc58336719]Additional General Information on Drinking Water
Drinking water, including bottled water, may reasonably be expected to contain at least small amounts of some contaminants.  The presence of contaminants does not necessarily indicate that the water poses a health risk.  More information about contaminants and potential health effects can be obtained by calling the U.S. EPA’s Safe Drinking Water Hotline (1-800-426-4791).
Some people may be more vulnerable to contaminants in drinking water than the general population.  Immuno-compromised persons such as persons with cancer undergoing chemotherapy, persons who have undergone organ transplants, people with HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections.  These people should seek advice about drinking water from their health care providers.  U.S. EPA/Centers for Disease Control (CDC) guidelines on appropriate means to lessen the risk of infection by Cryptosporidium and other microbial contaminants are available from the Safe Drinking Water Hotline (1-800-426-4791).
Lead can cause serious health problems, especially for pregnant women and young children. Lead in drinking water is primarily from materials and components associated with service lines and home plumbing. [NAME OF UTILITY] is responsible for providing high quality drinking water and removing lead pipes, but cannot control the variety of materials used in plumbing components in your home. You share the responsibility for protecting yourself and your family from the lead in your home plumbing. You can take responsibility by identifying and removing lead materials within your home plumbing and taking steps to reduce your family's risk. Before drinking tap water, flush your pipes for several minutes by running your tap, taking a shower, doing laundry or a load of dishes. You can also use a filter certified by an American National Standards Institute accredited certifier to reduce lead in drinking water. If you are concerned about lead in your water and wish to have your water tested, contact [NAME OF UTILITY and CONTACT INFORMATION]. Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available at http://www.epa.gov/safewater/lead.
[bookmark: _Toc58336720]Summary Information for Violation of a MCL, MRDL, AL, TT, or Monitoring and Reporting Requirement
Table 7. Violation of a MCL, MRDL, AL, TT or Monitoring Reporting Requirement
	Violation
	Explanation
	Duration
	Actions Taken to Correct Violation
	Health Effects Language

	None
	N/A
	N/A
	N/A
	N/A



[bookmark: _Toc58336721]For Water Systems Providing Groundwater as a Source of Drinking Water
Table 8.  Sampling Results Showing Fecal Indicator-Positive Groundwater Source Samples
	Microbiological Contaminants (complete if fecal-indicator detected)
	Total No. of Detections
	Sample Dates
	MCL [MRDL]
	PHG (MCLG) [MRDLG]
	Typical Source of Contaminant

	E. coli
	None
	Monthly
	0
	(0)
	Human and animal fecal waste

	Total Coliform
	None
	Monthly
	TT
	N/A
	Naturally occurring in the environment


[bookmark: _Toc58336725][bookmark: _Hlk58234306]Summary Information for Operating Under a Variance or Exemption
[bookmark: _Toc58336726]We are not operating under a variance or exemption.
Summary Information for Revised Total Coliform Rule Level 1 and Level 2 Assessment Requirements
We were not required to conduct a Level 1 or Level 2 Assessment in 2025 and the system is not in violation of the E. coli MCL.  
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