## 2022 Consumer Confidence Report

|  |  |  |  |
| --- | --- | --- | --- |
| Water System Name: | **Land Projects Mutual Water Company** | Report Date: | June 29, 2023 |

*We test the drinking water quality for many constituents as required by state and federal regulations. This report is revised and shows the results of our monitoring for the period of January 1 to December 31, 2021, and may include earlier monitoring data.*

**Este informe contiene información muy importante sobre su agua para beber. Favor de comunicarse Land Projects Mutual Water Company a 8810 West Avenue E-8, Antelope Acres, CA 93536 para asistirlo en español.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Type of water source(s) in use: | | Groundwater Wells | | | | | |
| Name & general location of source(s): | | | Wells 1, 3, and 8 | | | | |
| Drinking Water Source Assessment information: | | | | A source water assessment was conducted for Wells 1, 3, and in | | | |
| October 2001: For Well 8 in July 2009. A copy of the complete assessment may be viewed at the Company’s office located at 8810 West Avenue E-8, Antelope Acres, CA 93536 | | | | | | | |
| Time and place of regularly scheduled board meetings for public participation: | | | | | 2nd Tuesday of the month, at 6:00 p.m. | | |
| At the company office located at 8810 West Avenue E-8 Antelope Acres, CA 93536 | | | | | | | |
| For more information, contact: | John Houghton | | | | | Phone: | (661) 948-2550 |

|  |  |
| --- | --- |
| **TERMS USED IN THIS REPORT** | |
| **Maximum Contaminant Level (MCL)**: The highest level of a contaminant that is allowed in drinking water. Primary MCLs are set as close to the PHGs (or MCLGs) as is economically and technologically feasible. Secondary MCLs are set to protect the odor, taste, and appearance of drinking water.  **Maximum Contaminant Level Goal (MCLG)**: The level of a contaminant in drinking water below which there is no known or expected risk to health. MCLGs are set by the U.S. Environmental Protection Agency (U.S. EPA).  **Public Health Goal (PHG)**: The level of a contaminant in drinking water below which there is no known or expected risk to health. PHGs are set by the California Environmental Protection Agency.  **Maximum Residual Disinfectant Level (MRDL)**: The highest level of a disinfectant allowed in drinking water. There is convincing evidence that addition of a disinfectant is necessary for control of microbial contaminants.  **Maximum Residual Disinfectant Level Goal (MRDLG)**:The level of a drinking water disinfectant below which there is no known or expected risk to health. MRDLGs do not reflect the benefits of the use of disinfectants to control microbial contaminants.  **Primary Drinking Water Standards (PDWS)**: MCLs and MRDLs for contaminants that affect health along with their monitoring and reporting requirements, and water treatment requirements. | **Secondary Drinking Water Standards (SDWS)**:MCLs for contaminants that affect taste, odor, or appearance of the drinking water. Contaminants with SDWSs do not affect the health at the MCL levels.  **Treatment Technique (TT)**: A required process intended to reduce the level of a contaminant in drinking water.  **Regulatory Action Level (AL)**: The concentration of a contaminant which, if exceeded, triggers treatment or other requirements that a water system must follow.  **ND**: not detectable at testing limit **ppm**: parts per million or milligrams per liter (mg/L) **ppb**: parts per billion or micrograms per liter (µg/L) **ppt**: parts per trillion or nanograms per liter (ng/L)  **ppq**: parts per quadrillion or picogram per liter (pg/L) **pCi/L**: picocuries per liter (a measure of radiation) |

**The sources of drinking water** (both tap water and bottled water) include rivers, lakes, streams, ponds, reservoirs, springs, and wells. As water travels over the surface of the land or through the ground, it dissolves naturally-occurring minerals and, in some cases, radioactive material, and can pick up substances resulting from the presence of animals or from human activity.

**Contaminants that may be present in source water include:**

* *Microbial contaminants*, such as viruses and bacteria, that may come from sewage treatment plants, septic systems, agricultural livestock operations, and wildlife.
* *Inorganic contaminants*, such as salts and metals, can be naturally occurring or result from urban stormwater runoff, industrial or domestic wastewater discharges, oil and gas production, mining, or farming.
* *Pesticides and herbicides*, that may come from a variety of sources such as agriculture, urban stormwater runoff, and residential uses.
* *Organic chemical contaminants*, including synthetic and volatile organic chemicals, that are byproducts of industrial processes and petroleum production, and can also come from gas stations, urban stormwater runoff, agricultural application, and septic systems.
* *Radioactive contaminants*, that can be naturally occurring or be the result of oil and gas production and mining activities.

**In order to ensure that tap water is safe to drink**, the U.S. EPA and the State Board prescribe regulations that limit the amount of certain contaminants in water provided by public water systems. The U.S. Food and Drug Administration regulations and California law also establish limits for contaminants in bottled water that provide the same protection for public health.

**Tables 1, 2, 3, 4, 5, and 6 list all of the drinking water contaminants that were detected during the most recent sampling for the constituent**. The presence of these contaminants in the water does not necessarily indicate that the water poses a health risk. The State Board allows us to monitor for certain contaminants less than once per year because the concentrations of these contaminants do not change frequently. Some of the data, though representative of the water quality, is more than one year old. Any violation of an AL, MCL, MRDL, or TT is asterisked. Additional information regarding the violation is provided later in this report.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Table 1 – SAMPLING RESULTS SHOWING the detection of coliform bacteria | | | | | | | | | | | | |
| **Microbiological Contaminants** (complete if bacteria detected) | | **Highest No. of Detections** | | **No. of Months in Violation** | | MCL | | | | | **MCLG** | **Typical Source of Bacteria** |
|  | |  | |  | |  | | | | |  |  |
| Total Coliform Bacteria (state Total Coliform Rule) | | 0 | | 1 | | No samples Taken | | | | | 0 | Naturally present in the environment |
| Fecal Coliform or *E. coli* (state Total Coliform Rule) | | 0 | | 0 | | No Samples Taken | | | | | 0 | Human and animal fecal waste |
| *E. coli*  (Federal Revised Total Coliform Rule) | | 0 | | 0 | | (a) | | | | | 0 | Human and animal fecal waste |
| (a) Routine and repeat samples are total coliform-positive, and either is *E. coli*-positive or system fails to take repeat samples following *E. coli*-positive routine sample or system fails to analyze total coliform-positive repeat sample for *E. coli*. | | | | | | | | | | | | |
| Table 2 – SAMPLING RESULTS SHOWING THE detection of Lead and copper | | | | | | | | | | | | |
| Lead and Copper (complete if lead or copper detected in the last sample set) | **Sample Date** | | **No. of Samples Collected** | | **90th Percentile Level Detected** | | **No. Sites Exceeding AL** | **AL** | **PHG** | **No. of Schools Requesting Lead Sampling** | | **Typical Source of Contaminant** |
| Lead (ppb) | 2021 | | 10 | | ND | | 0 | 15 | 0.2 | N/A | | Internal corrosion of household water plumbing systems; discharges from industrial manufacturers; erosion of natural deposits |
| Copper (ppm) | 2021 | | 10 | | 0.22 | | 0 | 1.3 | 0.3 | Not applicable | | Internal corrosion of household plumbing systems; erosion of natural deposits; leaching from wood preservatives |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| TAble 3 – SAMPLING RESULTS FOR sodium and hardness | | | | | | | |
| **Chemical or Constituent** (and reporting units) | **Sample Date** | | **Level Detected** | **Range of Detections** | **MCL** | **PHG (MCLG)** | **Typical Source of Contaminant** |
| Sodium (ppm) | 2019-2020 | | 48.6 | 46-50 | None | None | Salt present in the water and is generally naturally occurring |
| Hardness (ppm) | 2019-2020 | | 176.6 | 150-190 | None | None | Sum of polyvalent cations present in the water, generally magnesium and calcium, and are usually naturally occurring |
| **TAble 4 – detection of contaminants with a Primary Drinking Water Standard** | | | | | | | |
| **Chemical or Constituent** (and reporting units) | | **Sample Date** | **Level Detected** | **Range of Detections** | **MCL [MRDL]** | **PHG (MCLG) [MRDLG]** | **Typical Source of Contaminant** |
| **Arsenic (ppb) (\*\*see table below on Page 5 for further info**) | | 2022 | 13.41 | 10-26 | 10 | 0.004 | **Erosion of natural deposits; runoff from orchards; glass and electronics production wastes** |
| Nickel (ug/L) | | 2019-2020 | ND | ND-12 | 100 | 12 | Nickel is a chemical element and abundant on earth, most notably the planet’s iron/nickel core. It is used in the manufacture of many alloys and products such as stainless steel, ceramic paint, jewelry, batteries, and coins. Nickel is released into the environment by power plants, metal factories and waste incinerators. It is also used in fertilizers and enters groundwater from farm runoff. |
| Fluoride (ppm) | | 2019-2020 | 0.37 | 0.25-0.56 | 2 | 1 | Erosion of natural deposits; water additive which promotes strong teeth; discharge from fertilizer and aluminum factories |
| Hexavalent Chromium | | 2019-2020 | 3.4 | 3.1-3.7 | --- | 0.02 | Discharge from electroplating factories, leather tanneries, wood preservation, chemical synthesis, refractory production, and textile manufacturing facilities; erosion of natural deposits |
| Nitrate, (as nitrogen-N)  (ppm) | | 2022 | 4.6 | 3.6-6.2 | 10 | 10 | Runoff and leaching from fertilizer use; leaching from septic tanks and sewage; erosion of natural deposits |
| Gross-Alpha Particle  Activity (pCi/l) | | 2019 | 5.3 | 5.3 | 15 | (0) | Erosion of natural deposits |
| Uranium (pCi/l) | | 2019 | 3.7 | 3.7 | 20 | 0.43 | Erosion of natural deposits |
| Contaminate (CCR units) | | Date | Average | Range | MCL | PHG  Or MCLG | Violation - Yes |
| Total Trihalomethanes-  TTHMS (ug/l | | 2022 | 83 | 40-125 | 80 | N/A | By- product of drinking water  Chlorination (in the distribution  System) |
| Haloacetic Acids (ug/l | | 2022 | ND | ND | 60 | N/A | By- product of drinking water  Chlorination (in the distribution  System) |
| Total Chlorine Residual  (mg/l) | | 2022 | 0.61 | 0.55 | [MRDL  =  4.0 (as)  Cl2 ] | [ MRDL =  4 (as Cl2 ) | Drinking water disinfectant added  For treatment (in the distribution  System) |
| **TAble 5 – detection of contaminants with a Secondary Drinking Water Standard** | | | | | | | |
| **Chemical or Constituent** (and reporting units) | | **Sample Date** | **Level Detected** | **Range of Detections** | **SMCL** | **PHG (MCLG)** | Typical Source of Contaminant |
| Chloride (ppm) | | 2019-2020 | 53.6 | 49-56 | 500 |  | Runoff/leaching from natural deposits; seawater influence |
| Specific Conductance  (uS/cm) | | 2019-2020 | 526 | 490-550 | 1600 |  | Substances that form ions when in water; seawater influence |
| Sulfate (ppm) | | 2019-2020 | 36.3 | 25-43 | 500 |  | Runoff/leaching from natural deposits; industrial wastes |
| Total Dissolved Solids-  TDS (ppm) | | 2019-2020 | 326 | 300-340 | 1000 |  | Runoff/leaching from natural deposits; industrial wastes |
| Odor-Threshold (units) | | 2019-2020 | 1 | 1 | 1.0 | 3.0 | Naturally-occurring organic materials |
| Turbidity (units) | | 2019-2020 | 0.23 | 0.3-0.4 | 5 |  | Soil runoff |
| **TAble 6 – detection of UNREGULATED CONTAMINANTS** | | | | | | | |
| **Chemical or Constituent** (and reporting units) | | **Sample Date** | **Level Detected** | **Range of Detections** | **Notification Level** | | **Health Effects Language** |
| Vanadium (ppb) | | 2019-2020 | 8.4 | 8.1-8.6 | 50 ppb | | Vanadium exposures resulted in developmental and reproductive effects in rats. |
| Boron (B) (ug/l) | | 2019-2020 | 466 | 310-720 | 1000 ppb | | Boron exposures resulted in decreased fetal weight (developmental effects) in newborn rats. |

**Additional General Information on Drinking Water**

Drinking water, including bottled water, may reasonably be expected to contain at least small amounts of some contaminants. The presence of contaminants does not necessarily indicate that the water poses a health risk. More information about contaminants and potential health effects can be obtained by calling the U.S. EPA’s Safe Drinking Water Hotline (1-800-426-4791).

Some people may be more vulnerable to contaminants in drinking water than the general population. Immuno-compromised persons such as persons with cancer undergoing chemotherapy, persons who have undergone organ transplants, people with HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections. These people should seek advice about drinking water from their health care providers. U.S. EPA/Centers for Disease Control (CDC) guidelines on appropriate means to lessen the risk of infection by *Cryptosporidium* and other microbial contaminants are available from the Safe Drinking Water Hotline (1-800-426-4791).

Lead-Specific Language: If present, elevated levels of lead can cause serious health problems, especially for pregnant women and young children. Lead in drinking water is primarily from materials and components associated with service lines and home plumbing. **Land Projects Mutual Water Company** is responsible for providing high quality drinking water but cannot control the variety of materials used in plumbing components. When your water has been sitting for several hours, you can minimize the potential for lead exposure by flushing your tap for 30 seconds to 2 minutes before using water for drinking or cooking. [If you do so, you may wish to collect the flushed water and reuse it for another beneficial purpose, such as watering plants.] If you are concerned about lead in your water, you may wish to have your water tested. Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available from the Safe Drinking Water Hotline (1-800-426-4791) or at <http://www.epa.gov/lead>.

Nitrate in drinking water at levels above 10 mg/L is a health risk for infants of less than six months of age. Such nitrate levels in drinking water can interfere with the capacity of the infant’s blood to carry oxygen, resulting in serious illness; symptoms include shortness of breath and blueness of the skin. Nitrate levels above 10 mg/L may also affect the ability of the blood to carry oxygen in other individuals, such as pregnant women and those with specific enzyme deficiencies. If you are caring for an infant, or you are pregnant, you should ask advice from your health care provider.

**Land Projects Mutual Water Company** did not monitor for Total Trihalomethanes and Haloacetic acids during August 2021. We also did not comply with the citation issued by the State Water Board during November 2021**. Land Projects Mutual Water Company** has instituted permanent internal control mechanisms to ensure that Total Trihalomethanes and Haloacetic acids are collected annually during the 2nd week of August and directives of citations are complied with. Please see table below summarizing violation(s).

**Summary Information for Violation of a MCL, MRDL, AL, TT,  
or Monitoring and Reporting Requirement**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **VIOLATION OF A MCL, MRDL, AL, TT, OR MONITORING AND REPORTING REQUIREMENT** | | | | |
| **Violation** | **Explanation** | **Duration** | **Actions Taken to Correct the Violation** | **Health Effects Language** |
| **We violated arsenic MCL in all four quarters of 2022.** | Well 1 arsenic running annual average (RAA) was 12.2 ppb, for 2022, and exceeded the arsenic MCL of 10 ppb.  Well 3 arsenic running annual average (RAA) was 17 ppb, for 2022, and exceeded the arsenic MCL of 10 ppb.  Well 8 arsenic running annual average (RAA) was 11 ppb, for 2022, and exceeded the arsenic MCL of 10 ppb. | All four quarters of 2022 | Drilled a new well, well 6  and will provide arsenic treatment. | Some people who drink water containing arsenic in excess of the MCL over many years may experience skin damage or circulatory system problems and may have an increased risk of getting cancer. |

**Summary Information for Violation of a MCL, MRDL, AL, TT,  
or Monitoring and Reporting Requirement**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **VIOLATION OF A MCL, MRDL, AL, TT, OR MONITORING AND REPORTING REQUIREMENT** | | | | |
| **Violation** | **Explanation** | **Duration** | **Actions Taken to Correct the Violation** | **Health Effects Language** |
| **Failure to monitor for**  **disinfection byproducts**  **for August 2022**  **Failure to monitor for total coliform for July 2022.** | Failed to monitor for  trihalomethanes and  Haloacetic acids  Failed to monitor for total coliform required per our approved monitoring plan**.** | Annual monitoring for  2022  For the month of July 2022  . | Continue to monitor as required by the State Water Resource Control Board.  Continue to monitor in the sample sequence required per our approved monitoring plan. | Some people who drink  water containing  trihalomethanes in  excess of the MCL over  many years may  experience liver, kidney,  or central nervous  system problems, and  may have an increased  risk of getting cancer.  Some people who drink  water containing  Haloacetic acids in  excess of the MCL over  many years may have an  increased risk of getting  cancer.  We are required to monitor your drinking water for specific contaminants on a regular basis. Results of regular monitoring are an indicator of whether or not your drinking water meets health standards. During the month of July 2022, we did not monitor for total coliform in the distribution system in accordance with the sample sequence required per our approved monitoring plan, and therefore cannot be sure of the quality of our drinking water during that time. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **VIOLATION OF A MCL, MRDL, AL, TT, OR MONITORING AND REPORTING REQUIREMENT** | | | | |
| **Violation** | **Explanation** | **Duration** | **Actions Taken to Correct the Violation** | **Health Effects Language** |
| **Failure to comply with the directives of the Citation issued by the State Water Board during November 2021** | **Failed to comply with the directives** | **Upon completion of directives**  . | We have revised and reissued a Consumer Confidence Report (CCR) for calendar year 2021 and included the Notice that during August 2021 we failed to monitor for trihalomethanes and  haloacetic acids. The revised CCR and Notice was mailed out to customers and posted at the Antelope Acres Market and at the Land Projects Mutual Water Company Office.  Continue to monitor and report as required by the State Water Resource Control Board. We will monitor for trihalomethanes and haloacetic acids during the second week of August 2023  We have instituted permanent internal control mechanisms to ensure trihalomethanes and  haloacetic acids are collected annually during the second week of August. | Some people who drink  water containing  trihalomethanes in  excess of the MCL over  many years may  experience liver, kidney,  or central nervous  system problems, and  may have an increased  risk of getting cancer.  Some people who drink  water containing  Haloacetic acids in  excess of the MCL over  many years may have an  increased risk of getting  cancer. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **VIOLATION OF A MCL, MRDL, AL, TT, OR MONITORING AND REPORTING REQUIREMENT** | | | | |
| **Violation** | **Explanation** | **Duration** | **Actions Taken to Correct the Violation** | **Health Effects Language** |
| **Failure to report for Disinfectants Third Quarter of 2022** | Failed to report Third Quarter Disinfectant Residual compliance**.**  **.** | One quarter in 2022 which is the Third Quarter of 2022**.**  . | Continue to report as required by the State Water Resource Control Board. | Additionally, we are required to report to the State Water Board for disinfectants in your drinking water within 10 days after the end of each quarter for determining disinfectant residual compliance. The reporting of disinfectants is used as an indicator of whether or not your drinking water meets health standards. During October 2022, we did not report for disinfectant residual compliance. |