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2024 Consumer Confidence Report
	Water System Name:
	Valley Creek MHP      #270-2405
	Report Date:
	6/15/2025


We test the drinking water quality for many constituents as required by state and federal regulations.  This report shows the results of our monitoring for the period of January 1 - December 31, 2024
Este informe contiene información muy importante sobre su agua potable.  Tradúzcalo ó hable con alguien que lo entienda bien.
	Type of water source(s) in use:  
	Groundwater well

	Name & location of source(s):  
	Two wells, one active and on stand-by located at the park

	

	

	Drinking Water Source Assessment information:
	N/A

	

	Time and place of regularly scheduled board meetings for public participation:
	There are no regularly scheduled 

	Meeting open to the public

	For more information, contact: 
	Howard Hugo
	  Phone: 
	( 831 ) 224-4846

	

	TERMS USED IN THIS REPORT

	Maximum Contaminant Level (MCL): The highest level of a contaminant that is allowed in drinking water.  Primary MCLs are set as close to the PHGs (or MCLGs) as is economically and technologically feasible.  Secondary MCLs are set to protect the odor, taste, and appearance of drinking water.
Maximum Contaminant Level Goal (MCLG): The level of a contaminant in drinking water below which there is no known or expected risk to health.  MCLGs are set by the U.S. Environmental Protection Agency (USEPA).
Public Health Goal (PHG): The level of a contaminant in drinking water below which there is no known or expected risk to health.  PHGs are set by the California Environmental Protection Agency.
Maximum Residual Disinfectant Level (MRDL):  The highest level of a disinfectant allowed in drinking water.  There is convincing evidence that addition of a disinfectant is necessary for control of microbial contaminants.
Maximum Residual Disinfectant Level Goal (MRDLG): The level of a drinking water disinfectant below which there is no known or expected risk to health.  MRDLGs do not reflect the benefits of the use of disinfectants to control microbial contaminants.
	Primary Drinking Water Standards (PDWS): MCLs and MRDLs for contaminants that affect health along with their monitoring and reporting requirements, and water treatment requirements.
Secondary Drinking Water Standards (SDWS):  MCLs for contaminants that affect taste, odor, or appearance of the drinking water.  Contaminants with SDWSs do not affect the health at the MCL levels.
Treatment Technique (TT):  A required process intended to reduce the level of a contaminant in drinking water.
Regulatory Action Level (AL): The concentration of a contaminant which, if exceeded, triggers treatment or other requirements that a water system must follow.
Variances and Exemptions:  Department permission to exceed an MCL or not comply with a treatment technique under certain conditions.
ND: not detectable at testing limit  
ppm: parts per million or milligrams per liter (mg/L)
ppb: parts per billion or micrograms per liter (ug/L)
ppt: parts per trillion or nanograms per liter (ng/L) 
ppq: parts per quadrillion or picogram per liter (pg/L)
pCi/L: picocuries per liter (a measure of radiation)


The sources of drinking water (both tap water and bottled water) include rivers, lakes, streams, ponds, reservoirs, springs, and wells.  As water travels over the surface of the land or through the ground, it dissolves naturally-occurring minerals and, in some cases, radioactive material, and can pick up substances resulting from the presence of animals or from human activity.
Contaminants that may be present in source water include:
· Microbial contaminants, such as viruses and bacteria, that may come from sewage treatment plants, septic systems, agricultural livestock operations, and wildlife.
· Inorganic contaminants, such as salts and metals, that can be naturally-occurring or result from urban stormwater runoff, industrial or domestic wastewater discharges, oil and gas production, mining, or farming.
· Pesticides and herbicides, that may come from a variety of sources such as agriculture, urban stormwater runoff, and residential uses.
· Organic chemical contaminants, including synthetic and volatile organic chemicals, that are by-products of industrial processes and petroleum production, and can also come from gas stations, urban stormwater runoff, agricultural application, and septic systems.
· Radioactive contaminants, that can be naturally-occurring or be the result of oil and gas production and mining activities.
In order to ensure that tap water is safe to drink, the USEPA and the state Department of Public Health (Department) prescribe regulations that limit the amount of certain contaminants in water provided by public water systems.  Department regulations also establish limits for contaminants in bottled water that provide the same protection for public health.
Tables 1, 2, 3, 4, 5, 7, and 8 list all of the drinking water contaminants that were detected during the most recent sampling for the constituent.  The presence of these contaminants in the water does not necessarily indicate that the water poses a health risk.  The Department allows us to monitor for certain contaminants less than once per year because the concentrations of these contaminants do not change frequently.  Some of the data, though representative of the water quality, are more than one year old.
	TABLE 1 – SAMPLING RESULTS SHOWING THE DETECTION OF COLIFORM BACTERIA

	Microbiological Contaminants
(complete if bacteria detected)
	Highest No. of Detections
	No. of months in violation
	MCL
	 MCLG
	Typical Source of Bacteria

	Total Coliform Bacteria
	(In a mo.)
0
	
0
	More than 1 sample in a month with a detection
	0
	Naturally present in the environment

	Fecal Coliform or E. coli
	(In the year)
0
	
0
	A routine sample and a repeat sample detect total coliform and either sample also detects fecal coliform or E. coli
	0
	Human and animal fecal waste

	TABLE 2 – SAMPLING RESULTS SHOWING THE DETECTION OF LEAD AND COPPER

	Lead and Copper
(complete if lead or copper detected in the last sample set)
	No. of samples collected
	90th percentile level detected
	No. sites exceeding AL
	AL
	PHG
	Typical Source of Contaminant

	Lead (ppb)
9/30/2023
	5
	ND
	0
	15
	0.2
	Internal corrosion of household water plumbing systems; discharges from industrial manufacturers; erosion of natural deposits

	Copper (mg/L)
9/30/2023
	5
	0.102
	0
	1300
	300
	Internal corrosion of household plumbing systems; erosion of natural deposits; leaching from wood preservatives

	TABLE 3 – SAMPLING RESULTS FOR SODIUM AND HARDNESS

	Chemical or Constituent (and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
	PHG
(MCLG)
	Typical Source of Contaminant

	Sodium (ppm)
	08-03-20
	80
	80
	none
	none
	Salt present in the water and is generally naturally occurring

	Hardness (ppm)
	08-03-20
	263
	263
	none
	none
	Sum of polyvalent cations present in the water, generally magnesium and calcium, and are usually naturally occurring


*Any violation of an MCL or AL is asterisked.  Additional information regarding the violation is provided later in this report.
	

TABLE 4 – DETECTION OF CONTAMINANTS WITH A PRIMARY DRINKING WATER STANDARD

	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
[MRDL]
	PHG
(MCLG)
[MRDLG]
	Typical Source of Contaminant

	Chromium(ug/L)
	3/5/2024
	ND
	ND
	50
	N/A
	Discharge from steel & pulp mills & chrome plating; erosion of natural deposits

	Fluoride(mg/L)
	12/9/2024
	2.2

	2.2

	2
	1
	Erosion of natural deposits; water additive that’s promotes strong teeth; discharge from fertilizer and aluminum factories

	Nickel(ug/L)
	3/5/2024
	ND
	5.0
	100
	.0012
	Erosion of natural deposits; discharge from metal factories.

	Barium(ug/L)
	       3/5/2024
	      26.9
	26.9
	1000
	2
	Discharge of oil drilling wastes & from metal refineries; erosion of natural deposits.

	Nitrate As N (mg/L)
	3/5/24
	    ND
	
	10
	
	

	Nitrite
Mg/L
	3/5/24
	     ND
	
	1
	
	

	Aluminum
UG/L
	3/5/2024
	ND
	
	1000
	
	

	Antimony, Total
UG/L
	3/5/2024
	ND
	
	6
	
	

	Arsenic
UG/L
	3/5/2024
	ND
	
	10
	
	

	Beryllium, Total
UG/L
	3/5/2024
	ND
	
	4
	
	

	Cadmium
UG/L
	3/5/2024
	ND
	
	5
	
	

	Chromium, Hex
	3/5/2024
	ND
	
	10
	
	

	Mercury
UG/L
	3/5/2024
	ND
	
	2
	
	

	Perchlorate
UG/L
	12/9/2024
	ND
	
	6
	
	

	Selenium
UG/L
	3/5/2024
	ND
	
	50
	
	

	Thallium, Total
UG/L
	3/5/2024
	ND
	
	2
	
	

	1,1,1-Trichloroethane
UG/L
	12/9/2024
	ND
	
	200
	
	

	1,1,2,2-Tetrachloroethane
UG/l
	12/9/2024
	ND
	
	1
	
	

	1,1,2-Trichloroethane
UG/L
	12/9/2024
	ND
	
	5
	
	

	1,1-Dichloroethane
UG/L
	12/9/2024
	ND
	
	5
	
	

	1,1-Dichloroethylene
UG/L
	12/9/2024
	ND
	
	6
	
	

	1,2,4-Trichlorobenzene
UG/L
	12/9/2024
	ND
	
	5
	
	

	0-Dichlorobenzene
UG/L
	12/9/2024
	ND
	
	600
	
	

	1,2-Dichloroethane
UG/L
	12/9/2024
	ND
	
	0.5
	
	

	1,2-Dichloropropane
UG/L
	12/9/2024
	ND
	
	5
	
	

	1,3-Dichloroproene
UG/L
	12/9/2024
	ND
	
	0.5
	
	

	P-Dichlorobenzene
UG/L
	12/9/2024
	ND
	
	5
	
	

	Benzene
UG/L
	12/9/2024
	ND
	
	1
	
	

	Carbon Tetrachloride
UG/L
	12/9/2024
	ND
	
	0.5
	
	

	CIS-1,2-Dichloroethylene
UG/L
	12/9/2024
	ND
	
	6
	
	

	Dichloromethane
UG/L
	12/9/2024
	ND
	
	5
	
	

	Ethylbenzene
UG/L
	12/9/2024
	ND
	
	300
	
	

	Methyl Tert-Butyl Ehter
UG/L
	12/9/2024
	ND
	
	13
	
	

	Chlorobenzene
UG/L
	12/9/2024
	ND
	
	70
	
	

	Styrene
UG/L
	12/9/2024
	ND
	
	100
	
	

	Tetrachloroethylene
UG/L
	12/9/2024
	ND
	
	5
	
	

	Toluene
UG/L
	12/9/2024
	ND
	
	150
	
	

	Trans-1,2-Dichloroethylene
UG/L
	12/9/2024
	ND
	
	10
	
	

	Trichloroethylene
UG/L
	12/9/2024
	ND
	
	5
	
	

	Trichlorofluoromethane
UG/L
	12/9/2024
	ND
	
	150
	
	

	Trichlorotrifluoroehtane
UG/L
	12/9/2024
	ND
	
	1200
	
	

	Vinyl Chloride
UG/L
	12/9/2024
	ND
	
	0.5
	
	

	Xylenes, Total
UG/L
	12/9/2024
	ND
	
	1750
	
	

	1,2,3-Trichloropropane
UG/L
	6/17/2024
	ND
	
	0.005
	
	

	2,4D
UG/L
	9/10/2024
	ND
	
	70
	
	

	Atrazine
UG/L
	9/10/2024
	ND
	
	1
	
	

	Diquat
UG/L
	9/10/2024
	ND
	
	20
	
	

	Simazine
UG/L
	9/10/2024
	ND
	
	4
	
	

	TABLE 5 – DETECTION OF CONTAMINANTS WITH A SECONDARY DRINKING WATER STANDARD

	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
	PHG
(MCLG)
	Typical Source of Contaminant

	Chloride(mg/L)
	2/20/2024
	52.0
	52.0
	500
	N/A
	Runoff/leaching from natural deposits; seawater influence

	Iron(ug/L)
	2/20/2024
	140
	70
	300
	N/A
	Leaching from natural deposits; industrial wastes

	Manganese(ug/L)
	2/20/2024
	49
	45
	50
	N/A
	Leaching from natural deposits

	Specific conductance(E.C.)
	2/20/2024
	863
	863
	1600
	N/A
	Substances that form ions when in water; seawater influence.

	Sulfate(mg/L)
	2/20/2024
	164
	160
	500
	N/A
	Runoff/leaching from natural deposits; industrial wastes.

	Total dissolved solids(mg/L)
	2/20/2024
	546
	546
	1000
	N/A
	Runoff/leaching from natural deposits

	Turbidity(NTU)
	2/20/2024
	1.40
	
	5
	N/A
	Soil Runoff

	Zinc(ug/L)
	2/20/2024
	10ND
	
	5000
	N/A
	Runoff/leaching from natural deposits; industrial wastes.

	Alkalinity, Bicarbonate
Mg/L
	2/20/2024
	259
	
	
	
	

	Calcium
Mg/L
	2/20/2024
	72
	
	
	
	

	Alkalinity, Carbonate
Mg/L
	2/20/2024
	ND
	
	
	
	

	Color
UNITS
	2/20/2024
	20.0
	
	15
	
	

	Foaming Agents
Surfactants
	2/20/2024
	ND
	
	
	
	

	    Copper, Free
UG/L
	3/5/2024
	ND
	
	1000
	
	

	Hardness as Calcium Carbonate
	2/20/2024
	266.0
	
	
	
	

	Hydroxide as Calcium Cabonate
	2/20/2024
	ND
	
	
	
	

	Magnesium
Mg/L
	2/20/2024
	20.8
	
	
	
	

	Odor
	2/20/2024
	ND
	
	3
	
	

	PH
	2/20/2024
	7.4
	
	
	
	

	Silver
UG/L
	2/20/2024
	ND
	
	100
	
	

	Sodium
Mg/L
	2/20/2024
	85.0
	
	
	
	

	Conductivity @ 25 C
UMHOS/CM
	2/20/2024
	863
	
	1600
	
	

	
	
	
	
	
	
	

	TABLE 6 – DETECTION OF UNREGULATED CONTAMINANTS

	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	Notification Level
	Health Effects Language

	
	
	
	
	
	

	
	
	
	
	
	


*Any violation of an MCL, MRDL, or TT is asterisked.  Additional information regarding the violation is provided later in this report.
Additional General Information on Drinking Water
Drinking water, including bottled water, may reasonably be expected to contain at least small amounts of some contaminants.  The presence of contaminants does not necessarily indicate that the water poses a health risk. More information about contaminants and potential health effects can be obtained by calling the USEPA’s Safe Drinking Water Hotline (1-800-426-4791).
Some people may be more vulnerable to contaminants in drinking water than the general population.  Immuno-compromised persons such as persons with cancer undergoing chemotherapy, persons who have undergone organ transplants, people with HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections. These people should seek advice about drinking water from their health care providers. USEPA/Centers for Disease Control (CDC) guidelines on appropriate means to lessen the risk of infection by Cryptosporidium and other microbial contaminants are available from the Safe Drinking Water Hotline (1-800-426-4791).
	Fluoride: Some people who drink water containing Fluoride in excess of the MCL of 4 mg/L over many years may get 

	bone disease; including pain and tenderness of the bones. Children who drink water containing Fluoride in excess of 

	the MCL of 2 mg/L may get mottled teeth.

	

	

	


Summary Information for Violation of a MCL, MRDL, AL, TT, 
or Monitoring and Reporting Requirement
	VIOLATION OF A MCL, MRDL, AL, TT, OR MONITORING AND REPORTING REQUIREMENT

	Violation
	Explanation
	Duration
	Actions Taken to Correct the Violation
	Health Effects Language

	Fluoride over MCL
	2.2 MG/L detected – MCL is 2.0 MG/L
	     12/9/2024
	Issue has been mitigated by installing POU R/O devices at each unit

Additionally, waiver was granted raising the Fluoride MCL to 3.0 Mg/L
	Some people who drink water containing Fluoride in excess of the MCL of 4 mg/L over many years may get bone disease, including pain and tenderness of the bones. Children who drink water containing Fluoride in excess of the MCL of 2 mg/L may get mottled teeth

	
	
	
	
	



For Water Systems Providing Ground Water as a Source of Drinking Water
	

TABLE 7 – SAMPLING RESULTS SHOWING
FECAL INDICATOR-POSITIVE GROUND WATER SOURCE SAMPLES

	Microbiological Contaminants
(complete if fecal-indicator detected)
	Total No. of Detections
	Sample
 Dates
	MCL
[MRDL]
	PHG
(MCLG)
[MRDLG]
	Typical Source of Contaminant

	E. coli
	0
	
	0
	(0)
	Human and animal fecal waste

	Enterococci
	0
	
	TT
	n/a
	Human and animal fecal waste

	Coliphage
	0
	
	TT
	n/a
	Human and animal fecal waste


Summary Information for Fecal Indicator-Positive Ground Water Source Samples,
Uncorrected Significant Deficiencies, or Ground Water TT 
	SPECIAL NOTICE OF FECAL INDICATOR-POSITIVE GROUND WATER SOURCE SAMPLE

	N/A

	

	

	

	

	SPECIAL NOTICE FOR UNCORRECTED SIGNIFICANT DEFICIENCIES

	N/A

	

	

	

	

	[bookmark: _Hlk280081436]VIOLATION OF GROUND WATER TT

	TT Violation
	Explanation
	Duration
	Actions Taken to Correct the Violation
	Health Effects Language

	N/A
	
	
	
	

	
	
	
	
	


For Systems Providing Surface Water as a Source of Drinking Water
	TABLE 8 - SAMPLING RESULTS SHOWING TREATMENT OF  SURFACE WATER SOURCES

	Treatment Technique (a)
(Type of approved filtration technology used)
	

	Turbidity Performance Standards (b)
(that must be met through the water treatment process)
	Turbidity of the filtered water must:
1 – Be less than or equal to _____ NTU in 95% of measurements in a month.
2 – Not exceed _____ NTU for more than eight consecutive hours.
3 – Not exceed ____ NTU at any time.

	Lowest monthly percentage of samples that met Turbidity Performance Standard No. 1.
	

	Highest single turbidity measurement during the year
	

	Number of violations of any surface water treatment requirements
	


(a)	A required process intended to reduce the level of a contaminant in drinking water.
(b)	Turbidity (measured in NTU) is a measurement of the cloudiness of water and is a good indicator of water quality and filtration performance.  Turbidity results which meet performance standards are considered to be in compliance with filtration requirements.
* Any violation of a TT is marked with an asterisk.  Additional information regarding the violation is provided below.
Summary Information for Violation of a Surface Water TT
	VIOLATION OF A SURFACE WATER TT

	TT Violation
	Explanation
	Duration
	Actions Taken to Correct the Violation
	Health Effects Language

	N/A
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Summary Information for Operating Under a Variance or Exemption 
	In 2024, a variance was granted, raising the Fluoride MCL from 2.0 to 3.0 Mg/L. POU devices are still being used and serviced in each residential unit for residents’ use.

	

	

	

	

	








	 
	 
