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2026 Annual Water Quality Report

Christopher Ranch L.L.C.                                                   Non-Transient / Non-Community

305 Bloomfield Ave., Gilroy, CA.  95020                                 Water System #: CA4300957

Christopher Ranch L.L.C. has prepared the following Annual Water Quality Report in an effort to keep our employees and users informed about the quality of the water supply.  This report outlines the water quality and what it means.  If anyone has any questions concerning the water quality or this report, please contact Jason Christopher at: (408) 848-9282.
Este informe contiene información muy importante sobre su agua beber.  
Tradúzcalo ó hable con alguien que lo entienda bien.
Christopher Ranch L.L.C. routinely monitors the drinking water quality for many constituents as required by State and Federal Regulations.  This report shows the results of our monitoring for the period of January 1 - December 31, 2025.

A source water assessment of the drinking water sources for Christopher Ranch was conducted in September 2003 for Well #1, in July 2012 for Well #2 and in May 2016 for the well at building AE. The sources are considered most vulnerable to the following activities not associated with any detected contaminants in the water supply: Automotive Repair, Metal Fabrication, Petroleum & Chemical Storage and Wastewater treatment plant operations. A copy of the assessment summary may be requested in the Christopher Ranch L.L.C. personnel office.

In this report you will find many terms and abbreviations that might not be familiar to you.  To help you better understand these terms we have provided the following definitions.

	

	TERMS USED IN THIS REPORT:

	Maximum Contaminant Level (MCL): The highest level of a contaminant that is allowed in drinking water.  Primary MCLs are set as close to the PHGs (or MCLGs) as is economically and technologically feasible.  Secondary MCLs are set to protect the odor, taste, and appearance of drinking water.

Maximum Contaminant Level Goal (MCLG): The level of a contaminant in drinking water below which there is no known or expected risk to health.  MCLGs are set by the U.S. Environmental Protection Agency (USEPA).

Regulatory Action Level (AL): The concentration of a contaminant which, if exceeded, triggers treatment or other requirements which a water system must follow.

Variances and Exemptions:  Department permission to exceed on MCL or not comply with treatment technique under certain conditions.
	Public Health Goal (PHG): The level of a contaminant in drinking water below which there is no known or expected risk to health.  PHGs are set by the California Environmental Protection Agency.

Primary Drinking Water Standards (PDWS): MCLs for contaminants that affect health along with their monitoring and reporting requirements, and water treatment requirements

Secondary Drinking Water Standards (SDWS):  MCLs for contaminants that affect taste, odor, or appearance of the drinking water.  Contaminants with SDWSs do not affect the health at the MCL levels.

ND: not detectable at testing limit

ppm: parts per million or milligrams per liter (mg/L)

ppb: parts per billion or micrograms per liter (ug/L)
ppt: parts per trillion or nanograms per liter (ng/L)

pCi/L: picocuries per liter (a measure of radiation)


The sources of drinking water (both tap water and bottled water) include rivers, lakes, streams, ponds, reservoirs, springs and wells.  As water travels over the surface of the land or through the ground, it dissolves naturally-occurring minerals and in some cases, radioactive material and can pick up substances resulting from the presence of animals or from human activity.

Contaminants that may be present in source water include:

· Microbial contaminants; such as viruses, and bacteria, that may come from sewage treatment plants, septic systems, agricultural livestock operations, and wildlife.

· Inorganic contaminants; such as salts and metals, that can be naturally-occurring or result from urban stormwater runoff, industrial or domestic wastewater discharges, oil and gas production, mining  or farming.

· Pesticides and herbicides; which may come from a variety of sources such as agriculture, urban stormwater runoff and residential uses.

· Organic chemical contaminants; including synthetic and volatile organic chemicals, that are byproducts of industrial processes and petroleum production, and can also come from gas stations, urban storm water runoff and septic systems.

· Radioactive contaminants; which can be naturally-occurring or be the result of oil and gas production and mining activities.

In order to ensure that tap water is safe to drink, USEPA and the California State Water Resource Control Board (State Board) prescribe regulations that limit the amount of certain contaminants in water provided by public water systems.  State Board regulations also establish limits for contaminants in bottled water that must provide the same protection for public health.
Tables 1, 2, 3, 4 and 5 list the drinking water contaminants that were detected during the most recent sampling for the constituent.  The presence of these contaminants in the water does not necessarily indicate that the water poses a health risk.  The State Board allows us to monitor for certain contaminants less than once per year because the concentrations of these contaminants are not expected to vary significantly from year to year.  Some of the data, though representative of the water quality, is more than a year old.    

	Table 1 – MONTHLY sampling results showing the detection of coliform bacteria

	Microbiological Contaminants


	Highest

No. of detections
	No. of months in violation
	MCL
	MCLG
	Typical Source of Bacteria

	Total Coliform Bacteria
	0
	0
	More than 1 sample in a month with a detection
	0
	Naturally present in the environment

	Fecal Coliform or 
E. coli
	0


	0
	A routine sample and a repeat sample detect total coliform and either sample also detects fecal coliform or E. coli
	0
	Human and animal fecal waste

	
	
	
	
	
	


	Table 2 – sampling results showing the detection of Lead and copper

	Lead and Copper

Sample Date:
	No. of samples collected
	90th percentile level detected
	No. Sites exceeding AL
	AL
	MCLG
	Typical Source of Contaminant

	Lead (ppm) 11/20/07

Lead (ppm) 10/20/08

Lead (ppm) 07/26/12

Lead (ppm) 09/28/15

Lead (ppm) 09/10/18

Lead (ppm) 07/30/21

Lead (ppm) 10/06/24
	10

10

10

10

10

10
10
	0.0054

0.0050

<0.005

0.0054

ND
ND

ND
	0

0

0

0

0

0
0
	0.015

0.015

0.015

0.015

0.015

0.015
0.015
	2

2

2

2

2

2
2
	Internal corrosion of household water plumbing systems; discharges from industrial manufacturers; erosion of natural deposits.

	Copper (ppm) 11/20/07

Copper (ppm) 10/20/08

Copper (ppm) 07/26/12

Copper (ppm) 09/28/15

Copper (ppm) 09/10/18
Copper (ppm) 07/30/21

Copper (ppm) 10/06/24
	10

10

10

10

10

10
10
	0.094

0.16

0.120

0.130

0.210
0.130

0.280
	0

0

0

0

0

0
0
	1.3

1.3

1.3

1.3

1.3

1.3
1.3
	0.17

0.17

0.17

0.17

0.17

0.17
0.17
	Internal corrosion of household water plumbing systems; erosion of natural deposits; leaching from wood preservatives.

	
	
	
	
	
	
	

	TAble 3 – sampling results for sodium and hardness

	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
	PHG

(MCLG)
	Typical Source of Contaminant

	Sodium (ppm)
	10/04/22

10/04/23

10/02/24

07/09/26
	35

34

34

33
	35

34

34

33
	None
	None
	Generally, found in ground and surface water

	Hardness (ppm)
	05/28/15
	313
	230-410
	None
	None
	Generally, found in ground and surface water


	TAble 4 – detection of contaminants with a Primary Drinking Water Standard

	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
	PHG

(MCLG)
	Typical Source of Contaminant

	Barium
	02/28/18

01/13/21
12/07/23
	33 ug/L
56.75 ug/L
50 ug/L
	ND-100ug/L
ND-170ug/L
ND-170ug/L
	1000 ug/L
	2000 ug/L
	Discharge of oil drilling wastes and from metal refineries; erosion of natural deposits

	Fluoride
	02/28/18
01/13/21
12/07/23
	0.3 mg/L
0.6 mg/L
ND
	ND-0.1 mg/L
ND-0.1 mg/L
ND-0.1mg/L
	2 mg/L
	4 mg/L
	Erosion of natural deposits; water additive that promotes strong teeth; discharge from fertilizer and aluminum factories

	Chromium (Total)
	02/28/18

01/13/21
12/07/23
	ND

ND
ND
	ND

ND
ND
	50 ug/L
	10 ug/L
	Discharge from electroplating factories, leather tanneries, wood preservation, chemical synthesis, refractory production and textile manufacturing facilities

	Nitrate (as N)
	12/07/23

10/02/24

01/07/25

04/09/26
	2.8 mg/L

2.8 mg/L

2.7 mg/L

3.1 mg/L
	2.8 mg/L

3.4-3.7 mg/L

2.7 mg/L

3.1 mg/L
	10 mg/L


	10 mg/L
	Runoff and leaching from fertilizer use; leaching from septic tanks, sewage; erosion of natural deposits

	Perchlorate
	02/25/25

04/23/26
	ND

ND
	ND-ND

ND-ND
	0.006 mg/L
	0.006 mg/L
	Perchlorate is an inorganic chemical used in solid rocket propellant, fireworks, explosives, flares, matches & a variety of industries.

	Trichloropropane-1,2,3
	09/23/21

02/25/25
	ND
ND
	ND-ND
ND-ND
	0.0050 ug/L
	
	1,2,3- TCP is a chlorinated hydrocarbon with high chemical stability. It is a manmade chemical found at industrial or hazardous waste sites. It has been used as a cleaning and degreasing solvent and also is associated with pesticide products.


*Any violation of an MCL or AL is asterisked.  Additional information regarding the violation is provided on the next page.
	TAble 5 – detection of contaminants with a Secondary Drinking Water Standard

	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
	PHG

(MCLG)
	Typical Source of Contaminant

	Chloride
	10/04/23

04/08/24

10/2/24
04/09/26
	41 mg/L
25 mg/L
40 mg/L

39 mg/L
	

	500-600 mg/L
	N/A
	Runoff/leaching from natural deposits; seawater influence

	Specific Conductance

Micromhos
	04/23/19
03/16/22

02/25/25
	715 mg/L
660 mg/L
600 mg/L
	570-860
	1,600-2,200 µS/cm
	N/A
	Substances that form ions when in water; seawater influence

	Sulfate
	0/04/23

04/08/24

10/02/24
04/09/26
	42 mg/L
37 mg/L

 42 mg/L

40 mg/L
	

	500-600 mg/L
	N/A
	Runoff/leaching from natural deposits’ industrial wastes

	Total Dissolved Solids
	10/04/23

04/08/24

10/02/24

04/09/26
	320 mg/L
320 mg/L
390 mg/L
410 mg/L
	330
320

320

390
	1000-1500 mg/L
	N/A
	Runoff/leaching from natural deposits

	Turbidity
	10/04/18
	1.29 units
	
	5 units
	N/A
	Soil runoff

	Aluminum
	02/28/18

01/13/21
12/07/23
	ND

ND
ND
	ND

ND
ND
	200 ug/L
	N/A
	Erosion of natural deposits; residual from some surface water treatment processes

	Iron
	06/25/19
05/12/21

12/07/23
	ND
ND
ND
	ND
ND
ND
	300 µg/L
	N/A
	Leaching from natural deposits; industrial wastes


*Any violation of an MCL or AL is asterisked.  Additional information regarding the violation is provided below.

Additional General Information on Drinking Water

All drinking water, including bottled water, may reasonably be expected to contain at least small amounts of some contaminants.  The presence of contaminants does not necessarily indicate that the water poses a health risk. More information about contaminants and potential health effects can be obtained by calling the USEPA’s Safe Drinking Water Hotline (1-800-426-4791).

Some people may be more vulnerable to contaminants in drinking water than the general population.  Immuno-compromised persons such as persons with cancer undergoing chemotherapy, persons who have undergone organ transplants, people with HIV/AIDS or other immune system disorders, some elderly, and infants, can be particularly at risk from infections. These people should seek advice about drinking water from their health care providers. USEPA/Centers for Disease Control (CDC) guidelines on appropriate means to lessen the risk of infection by Cryptosporidium and other microbial contaminants are available from the Safe Drinking Water Hotline (1-800-426-4791).

	

	

	


Report prepared by: Rory Raggio




Date of Report: August 4th, 2026

System Operator: Jason Christopher

	IMPORTANT Christopher Ranch (CA4300957) Has Detected Levels of Perfluorooctanoic Acid (PFOA) Above the “Notification Level”


Christopher Ranch routinely monitors the water system for the presence of contaminants.  In July 2026, the Christopher Ranch water system confirmed a concentration of PFOA/PFOS above the public health-based notification level in its raw water.  Subsequent testing confirmed that the filtration systems installed on Christopher Ranch drinking fountains are effectively removing all detectable PFOA and PFOS contaminants.

What should I do?
· You do not need to use an alternative (e.g., bottled) water supply.

· This is not an immediate risk. If it had been, you would have been notified immediately. However, some people who drink water containing PFOA in excess of the notification level over many years may experience adverse health effects. PFOA exposures have been shown to cause increased liver weight and cancer in laboratory animals. 
· If you have other health issues concerning the consumption of this water, you may wish to consult your personal physician.

What is being done?

Well #2, which had the highest test results, (exceeding the response level established by the California Division of Drinking water) has been taken offline and locked out.

All Christopher Ranch drinking fountains are equipped with reverse osmosis (RO) filtration systems. We have tested the water from these drinking fountains and confirmed that the RO systems are effectively removing PFOS and PFOA contaminants. Reverse osmosis filtration systems have also been installed on the coffee machines in Building S to ensure that drinking water used for coffee preparation is similarly free of PFOS and PFOA.

Christopher Ranch is actively working with the State Water Resources Control Board and multiple water engineering firms to evaluate and implement long-term treatment solutions for our water system.  We are committed to achieving full compliance and anticipate resolving the issue well before the federal deadline in 2029.

For more information, please contact Human Resources at; HR@ChristopherRanch.com or (408) 848-9241

	Christopher Ranch (CA4300957) Ha Detectado Niveles De Acido Perfluorooctanoico (PFOA) Por Encima Del "Nivel de Notificación"


Christopher Ranch monitorea de manera rutinaria su sistema de agua para detectar la presencia de contaminantes. En julio de 2026, el sistema de agua de Christopher Ranch confirmó una concentración de PFOA/PFOS por encima del Nivel de Notificación establecido para proteger la salud pública.  Pruebas posteriores confirmaron que los sistemas de filtración instalados en los bebederos de Christopher Ranch están eliminando eficazmente todos los contaminantes detectables de PFOA y PFOS.

¿Qué debo hacer?

· No necesita utilizar una fuente alternativa de agua (por ejemplo, agua embotellada).

· Esto no representa un riesgo inmediato para la salud. Si hubiera existido un riesgo inmediato, se le habría notificado de inmediato. Sin embargo, las personas que consumen agua con niveles de PFOA superiores al Nivel de Notificación durante muchos años podrían experimentar efectos adversos para la salud. En estudios de laboratorio, la exposición al PFOA ha demostrado causar aumento del peso del hígado y cáncer en animales.
· Si tiene otras inquietudes de salud relacionadas con el consumo de esta agua, puede consultar con su médico personal.¿Qué se está haciendo?
El Pozo n.º 2, que presentó los resultados más altos en las pruebas (superando el nivel de respuesta establecido por la División de Agua Potable de California), ha sido puesto fuera de servicio y bloqueado.
Todos los bebederos de Christopher Ranch están equipados con sistemas de filtración por ósmosis inversa (RO). Hemos analizado el agua de estos bebederos y confirmado que los sistemas de ósmosis inversa eliminan eficazmente los contaminantes PFOS y PFOA. Además, se han instalado sistemas de ósmosis inversa en las cafeteras del Edificio S para garantizar que el agua utilizada para preparar café también esté libre de PFOS y PFOA.

Christopher Ranch está trabajando activamente con la Junta Estatal de Control de los Recursos Hídricos de California y con varias empresas de ingeniería especializadas en sistemas de agua para evaluar e implementar soluciones de tratamiento a largo plazo para nuestro sistema de agua. Estamos comprometidos a cumplir plenamente con todos los requisitos reglamentarios y anticipamos resolver este asunto mucho antes de la fecha límite establecida por el Estado para 2029.

Para obtener más información, comuníquese con el Departamento de Recursos Humanos: HR@ChristopherRanch.com or (408) 848-9241

	Sample

ID
	Sample

Name
	Sample

Date/Time


	Result
	Analyte
	Units
	MCL
	Notification
	Action Level

	AJG0320-01
	WELL 02 - OLD WELL
	Jun 30 2026 11:55AM
	4.6
	PFHxS
	ng/L
	10
	3
	10

	AJG0320-01
	WELL 02 - OLD WELL
	Jun 30 2026 11:55AM
	27
	PFOA
	ng/L
	4
	4
	10

	AJG0320-01
	WELL 02 - OLD WELL
	Jun 30 2026 11:55AM
	44
	PFOS
	ng/L
	4
	4
	40

	AJG0320-02
	WELL 01 - NEW WELL
	Jun 30 2026 10:40AM
	7.6
	PFOA
	ng/L
	4
	4
	10

	AJG0320-02
	WELL 01 - NEW WELL
	Jun 30 2026 10:40AM
	12
	PFOS
	ng/L
	4
	4
	40

	AJG0320-03
	WELL 03 - AE WELL
	Jun 30 2026 11:45AM
	3.3
	PFHxS
	ng/L
	10
	3
	10

	AJG0320-03
	WELL 03 - AE WELL
	Jun 30 2026 11:45AM
	14
	PFOA
	ng/L
	4
	4
	10

	AJG0320-03
	WELL 03 - AE WELL
	Jun 30 2026 11:45AM
	19
	PFOS
	ng/L
	4
	4
	40
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