[bookmark: _jithq5hp97dc]The Ponderosa CSD provides water from 4 (four) wells with submersible pumps. Holby 1 and 2, Lake and Fawn wells are located within or adjacent to the Ponderosa subdivision. The Ponderosa CSD board of directors meets regularly on the second Thursday of each month in the district building, 56827 Aspen Dr, Springville, CA 93265. These meetings are open to the public. For more information contact the board secretary by email at secretary@ponderosacsd.com 
PCSD tests the drinking water quality for many constituents as required by state and federal regulations.  This report shows the results of our monitoring for the period of January 1 to December 31, 2025.

Este informe contiene información muy importante sobre su agua para beber.  Favor de comunicarse Ponderosa CSD a 56827 Aspen Dr, Springville, CA 93265, o email secretary@ponderosacsd.com para asistirlo es en español.
	Term
	Definition

	Level 1 Assessment
	A Level 1 assessment is a study of the water system to identify potential problems and determine (if possible) why total coliform bacteria have been found in our water system.

	Level 2 Assessment
	A Level 2 assessment is a very detailed study of the water system to identify potential problems and determine (if possible) why an E. coli MCL violation has occurred and/or why total coliform bacteria have been found in our water system on multiple occasions.

	Maximum Contaminant Level (MCL)
	The highest level of a contaminant that is allowed in drinking water. Primary MCLs are set as close to the PHGs (or MCLGs) as is economically and technologically feasible. Secondary MCLs are set to protect the odor, taste, and appearance of drinking water.

	Maximum Contaminant Level Goal (MCLG)
	The level of a contaminant in drinking water below which there is no known or expected risk to health. MCLGs are set by the U.S. Environmental Protection Agency (U.S. EPA).

	Maximum Residual Disinfectant Level (MRDL)
	The highest level of a disinfectant allowed in drinking water. There is convincing evidence that addition of a disinfectant is necessary for control of microbial contaminants.

	Maximum Residual Disinfectant Level Goal (MRDLG)
	The level of a drinking water disinfectant below which there is no known or expected risk to health. MRDLGs do not reflect the benefits of the use of disinfectants to control microbial contaminants.

	Primary Drinking Water Standards (PDWS)
	MCLs and MRDLs for contaminants that affect health along with their monitoring and reporting requirements, and water treatment requirements.

	Public Health Goal
(PHG)
	The level of a contaminant in drinking water below which there is no known or expected risk to health. PHGs are set by the California Environmental Protection Agency.

	Regulatory Action Level
(AL)
	The concentration of a contaminant which, if exceeded, triggers treatment or other requirements that a water system must follow.

	Secondary Drinking Water Standards (SDWS)
	MCLs for contaminants that affect taste, odor, or appearance of the drinking water. Contaminants with SDWSs do not affect the health at the MCL levels.

	Treatment Technique
(TT)
	A required process intended to reduce the level of a contaminant in drinking water.

	Variances and Exemptions
	Permissions from the State Water Resources Control Board (State Board) to exceed an MCL or not comply with a treatment technique under certain conditions.

	ND
	Not detectable at testing limit.

	ppm
	parts per million or milligrams per liter (mg/L)

	ppb
	parts per billion or micrograms per liter (µg/L)

	ppt
	parts per trillion or nanograms per liter (ng/L)

	ppq
	parts per quadrillion or picogram per liter (pg/L)

	pCi/L
	picocuries per liter (a measure of radiation)



The sources of drinking water (both tap water and bottled water) include rivers, lakes, streams, ponds, reservoirs, springs, and wells. As water travels over the surface of the land or through the ground, it dissolves naturally occurring minerals and, in some cases, radioactive material, and can pick up substances resulting from the presence of animals or from human activity. Contaminants that may be present in source water include:
Microbial contaminants, such as viruses and bacteria, that may come from sewage treatment plants, septic systems, agricultural livestock operations, and wildlife. Inorganic contaminants, such as salts and metals, can be naturally occurring or result from urban stormwater runoff, industrial or domestic wastewater discharges, oil and gas production, mining, or farming. Pesticides and herbicides, which may come from a variety of sources such as agriculture, urban stormwater runoff, and residential uses. Organic chemical contaminants, including synthetic and volatile organic chemicals, which are byproducts of industrial processes and petroleum production, and can also come from gas stations, urban stormwater runoff, agricultural application, and septic systems. Radioactive contaminants, which can be naturally occurring or be the result of oil and gas production and mining activities.
Regulation of Drinking Water and Bottled Water Quality
[bookmark: _s1sgp3czijoz]To ensure that tap water is safe to drink, the U.S. EPA and the State Board prescribe regulations that limit the amount of certain contaminants in water provided by public water systems. The U.S. Food and Drug Administration regulations and California law also establish limits for contaminants in bottled water that provide the same protection for public health.
[bookmark: _t32qg8abws6y]
[bookmark: _4hg8ylbc6q5h]2025 Consumer Confidence Report
[bookmark: _1vdeyypecnj3]Lake well with high Radon levels is currently shut off as we seek proper treatment
[bookmark: _bp32qu1t62ut]Tables 1, 2, 3, 4, and 5 list all the drinking water contaminants that were detected during the most recent sampling for the constituent. The presence of these contaminants in the water does not necessarily indicate that the water poses a health risk. The State Board allows us to monitor for certain contaminants less than once per year because the concentrations of these contaminants do not change frequently. Some of the data, though representative of the water quality, is more than one year old.
Table 1. Sampling Results Showing the Detection of Coliform Bacteria
	Microbiological Contaminants 
	Highest No. of Detections
	No. of Months in Violation
	MCL
	MCLG
	Typical Source of Bacteria

	E. coli

	(In the year)
0
	[Enter No.]
0
	(a)
	0
	Human and animal fecal waste


Table 2. Sampling Results Showing the Detection of Lead and Copper
	Lead and Copper 
	Sample Date
	No. of Samples Collected
	90th Percentile Level Detected
	No. Sites Exceeding AL
	AL
	PHG
	Typical Source of Contaminant

	Lead (ppb)
	03/24/2025
	10
	0
	0
	15
	0.2
	Internal corrosion of household water plumbing systems; discharges from industrial manufacturers; erosion of natural deposits

	Copper (ppm)
	03/24/2025
	10
	0
	0
	1.3
	0.3
	Internal corrosion of household plumbing systems; erosion of natural deposits; leaching from wood preservatives


Table 3. Sampling Results for Sodium and Hardness
	Chemical or Constituent (and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
	PHG (MCLG)
	Typical Source of Contaminant

	Sodium (ppm)
	03-24-2025
	6
	4-7
	None
	None
	Salt present in the water and is generally naturally occurring

	Hardness (ppm)
	03-24-2025
	40.28
	26.6-52.3
	None
	None
	Sum of polyvalent cations present in the water, generally magnesium and calcium, and are usually naturally occurring


Table 4. Detection of Contaminants with a Primary Drinking Water Standard
	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL [MRDL]
	PHG (MCLG) [MRDLG]
	Typical Source of Contaminant

	Nitrate
(as Nitrate, N) ppm
	03-24-2025
	0
	0
	45
	45
	Runoff and leaching from fertilizer use; leaching from septic tanks and sewage; erosion of natural deposits

	Nitrite (mg/L)
	03-24-2025
	0
	0
	1
	1
	Runoff and leaching from fertilizer use; leaching from septic tanks and sewage; erosion of natural deposits

	Fluoride (mg/L)
	03-24-2025
	0.05
	0-0.2 
	2 
	1 
	Erosion of natural deposits; water additive which promotes strong teeth; discharge from fertilizer and aluminum factories 

	Turbidity NTU
	03-24-2025
	0.325
	.15-.40
	5
	
	Soil runoff

	Gross Alpha
	07/15/2024
	4.67
	2.64-6.70
	15
	0
	Erosion of natural deposits

	Uranium 
	07/15/2024
	2.69
	2.69
	20
	.43
	Erosion of natural deposits


Table 5. Detection of Contaminants with a Secondary Drinking Water Standard
	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	SMCL
	PHG (MCLG)
	Typical Source of Contaminant

	Chloride mg/L
	03-24-2025
	1.5
	0-3
	500 mg/L
	500 mg/L
	Runoff/leaching from natural deposits; seawater influence

	Conductivity µS/cm

	03-24-2025
	120
	86-146
	1,600 µS/cm
	1,600 µS/cm
	Substances that form ions when in water; seawater influence

	Sulfate mg/L
	03-24-2025
	2.4
	0.7-5
	500 mg/L
	500 mg/L
	Runoff/leaching from natural deposits; industrial wastes

	Color units
	03-24-2025
	0
	0
	15units
	15 Units
	Naturally occurring organic materials

	Total Dissolved Solids (TDS)
	03-24-2025
	65
	50-90
	1,000 mg/L
	1,000 mg/L
	Runoff/leaching from natural deposits

	Foaming Agents (MBAS) (μg/L) 
	04-14-2025
	.05 
	.05 
	500 
	
	Municipal and industrial waste discharges 

	Iron
	03-24-2025
	27.5
	30-80
	
	
	

	Zinc
	03-24-2025
	20
	10-40
	
	
	

	               Radon
	11-24-2025
	Holby1 4040
	Holby2 4660
	Fawn 3450
	Lake 14800
	No current MCL           Lake well has been shut down









