2025 Consumer Confidence Report
Water System Name:	Countryside Care Center	Report Date:	06/27/2026
We test the drinking water quality for many constituents as required by state and federal regulations. This report shows the results of our monitoring for the period of January 1 to December 31, 2025 and may include earlier monitoring data.
Este informe contiene información muy importante sobre su agua para beber. Favor de comunicarse Countryside Care Center a 559-275-4785 / 925 N. Cornelia Fresno, CA para asistirlo en español.
Type of water source(s) in use:	 Groundwater	 Name & general location of source(s):	 Well 02 is located on the property at 925 N. Cornelia Fresno, CA	

Drinking Water Source Assessment information:	 The source is considered most vulnerable to the following activities not  associated with any detected contaminants: septic systems – low density [<1/acre], wells – agricultural/irrigation. The Water System is located in an agricultural area of the San Joaquin Valley and is susceptible to a wide variety of contaminants with agriculture. The system drilled a new well in 2001. Water analysis has been completed for the new source and results have

been acceptable. There have been no other contaminants detected in the water supply, however the source is still considered vulnerable to activities located near the drinking water source. Potential contamination could come from the septic systems and agricultural wells in the area.
Time and place of regularly scheduled board meetings for public participation:	 Please call for an appointment	

For more information, contact:	Coty Rivera	Phone:	559-420-1534

TERMS USED IN THIS REPORT

SWS CCR Form
Revised May 2025

Maximum Contaminant Level (MCL): The highest level of a contaminant that is allowed in drinking water. Primary MCLs are set as close to the PHGs (or MCLGs) as is economically and technologically feasible. Secondary MCLs are set to protect the odor, taste, and appearance of drinking water.
Maximum Contaminant Level Goal (MCLG): The level of a contaminant in drinking water below which there is no known or expected risk to health. MCLGs are set by the U.S. Environmental Protection Agency (U.S. EPA).
Public Health Goal (PHG): The level of a contaminant in drinking water below which there is no known or expected risk to health. PHGs are set by the California Environmental Protection Agency.
Maximum Residual Disinfectant Level (MRDL): The highest level of a disinfectant allowed in drinking water. There is convincing evidence that addition of a disinfectant is necessary for control of microbial contaminants.
Maximum Residual Disinfectant Level Goal (MRDLG): The level of a drinking water disinfectant below which there is no known or expected risk to health. MRDLGs do not reflect the benefits of the use of disinfectants to control microbial contaminants.
Primary Drinking Water Standards (PDWS): MCLs and MRDLs for contaminants that affect health along with their monitoring and reporting requirements, and water treatment requirements.

Secondary Drinking Water Standards (SDWS): MCLs for contaminants that affect taste, odor, or appearance of the drinking water. Contaminants with SDWSs do not affect the health at the MCL levels.
Treatment Technique (TT): A required process intended to reduce the level of a contaminant in drinking water.
Regulatory Action Level (AL): The concentration of a contaminant which, if exceeded, triggers treatment or other requirements that a water system must follow.
Variances and Exemptions: Permissions from the State Water Resources Control Board (State Board) to exceed an MCL or not comply with a treatment technique under certain conditions.
Level 1 Assessment: A Level 1 assessment is a study of the water system to identify potential problems and determine (if possible) why total coliform bacteria have been found in our water system.
Level 2 Assessment: A Level 2 assessment is a very detailed study of the water system to identify potential problems and determine (if possible) why an E. coli MCL violation has occurred and/or why total coliform bacteria have been found in our water system on multiple occasions.
ND: not detectable at testing limit
ppm: parts per million or milligrams per liter (mg/L) ppb: parts per billion or micrograms per liter (µg/L) ppt: parts per trillion or nanograms per liter (ng/L) ppq: parts per quadrillion or picogram per liter (pg/L) pCi/L: picocuries per liter (a measure of radiation)


The sources of drinking water (both tap water and bottled water) include rivers, lakes, streams, ponds, reservoirs, springs, and wells. As water travels over the surface of the land or through the ground, it dissolves naturally-occurring minerals and, in some cases, radioactive material, and can pick up substances resulting from the presence of animals or from human activity.
Contaminants that may be present in source water include:
· Microbial contaminants, such as viruses and bacteria, that may come from sewage treatment plants, septic systems, agricultural livestock operations, and wildlife.
· Inorganic contaminants, such as salts and metals, that can be naturally-occurring or result from urban stormwater runoff, industrial or domestic wastewater discharges, oil and gas production, mining, or farming.
· Pesticides and herbicides, that may come from a variety of sources such as agriculture, urban stormwater runoff, and residential uses.
· Organic chemical contaminants, including synthetic and volatile organic chemicals, that are byproducts of industrial processes and petroleum production, and can also come from gas stations, urban stormwater runoff, agricultural application, and septic systems.
· Radioactive contaminants, that can be naturally-occurring or be the result of oil and gas production and mining activities.
In order to ensure that tap water is safe to drink, the U.S. EPA and the State Board prescribe regulations that limit the amount of certain contaminants in water provided by public water systems. The U.S. Food and Drug Administration regulations and California law also establish limits for contaminants in bottled water that provide the same protection for public health.
Tables 1, 2, 3, 4, 5, and 6 list all of the drinking water contaminants that were detected during the most recent sampling for the constituent. The presence of these contaminants in the water does not necessarily indicate that the water poses a health risk. The State Board allows us to monitor for certain contaminants less than once per year because the concentrations of these contaminants do not change frequently. Some of the data, though representative of the water quality, are more than one year old. Any violation of an AL, MCL, MRDL, or TT is asterisked. Additional information regarding the violation is provided later in this report.


	TABLE 1 – SAMPLING RESULTS SHOWING THE DETECTION OF COLIFORM BACTERIA

	Microbiological Contaminants
	Highest No. of Detections
	No. of Months in Violation
	MCL
	MCLG
	Typical Source of Bacteria

	E. Coli
	0
	0
	1+
	0
	Human and animal fecal waste

	(a) Routine and repeat samples are total coniform-positive and either is E. coli-positive or system fails to take repeat samples following E. Coli-positive routine sample or system fails to analyze total coliform-positive repeat samples for E-coli.

	TABLE 1.A. - COMPLIANCE WITH TOTAL COLIFORM MCL BETWEEN JANUARY 1, 2023 AND JUNE 30, 2023 (INCLUSIVE)

	Microbiological Contaminants
	Highest No. of Detections
	No. of Months in Violation
	MCL
	MCLG
	Typical Source of Bacteria

	Total Coliform Bacteria
	0
	0
	1 positive monthly sample (a)
	0
	Naturally present in the environment

	Fecal Coliform and E.coli
	0
	0
	0
	None
	Human and animal fecal waste

	(a) For systems collecting fewer than 40 samples per month: two or more positively monthly samples is a violation of the total coliform MCL. For violation of the total coliform MCL, include potential adverse health effects, and actions taken by water system to address the violation: [Enter information]
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	TABLE 2 – SAMPLING RESULTS SHOWING THE DETECTION OF LEAD AND COPPER

	Lead and Copper (complete if lead or copper detected in the last sample set)
	Sample Date
	No. of Samples Collected
	90th Percentile
Level Detected
	No. Sites Exceeding AL
	
AL
	
PHG
	No. of Schools Requesting Lead
Sampling
	
Typical Source of Contaminant

	
Lead (ppb)
	
9/5/23
	
5
	
0.00
	
0
	
15
	
0.2
	
Not applicable
	Internal corrosion of household water plumbing systems; discharges from industrial manufacturers; erosion of
natural deposits

	
Copper (ppm)
	
9/5/23
	
5
	
0.00
	
0
	
1.3
	
0.3
	
Not applicable
	Internal corrosion of household plumbing systems; erosion of natural deposits; leaching from wood
preservatives



	TABLE 3 – SAMPLING RESULTS FOR SODIUM AND HARDNESS

	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
	PHG (MCLG)
	Typical Source of Contaminant

	Sodium (ppm)
	2023
	16
	NA
	None
	None
	Salt present in the water and is generally naturally occurring

	
Hardness (ppm)
	
2023
	
86
	
NA
	
None
	
None
	Sum of polyvalent cations present in the water, generally magnesium and
calcium, and are usually naturally occurring



	TABLE 4 – DETECTION OF CONTAMINANTS WITH A PRIMARY DRINKING WATER STANDARD

	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
[MRDL]
	PHG (MCLG) [MRDLG]
	
Typical Source of Contaminant

	*Arsenic
	2023
	2.5
	NA
	10
	.004
	Erosion of natural deposits; runoff from orchards; glass and electronics production wastes

	**Nitrate as N (ppm)
	2025
	3.6
	NA
	10
	10
	Runoff and leaching from fertilizer use; leaching from septic tanks and sewage; erosion of natural deposits

	Hex Chromium 
	2025
	3.2
	NA
	10
	0.02
	Erosion of natural deposits; transformation of
naturally occurring trivalent chromium to hexavalent chromium by natural processes and human activities
such as discharges from electroplating factories, leather tanneries, wood preservation, chemical synthesis, refractory production, and textile manufacturing facilities

	Fluoride 
	2023
	0.11
	N/A
	2
	1
	Some people who drink water containing fluoride in excess of the federal MCL of 4 mg/L over many
years may get bone disease, including pain and tenderness of the bones. Children who drink water containing fluoride in excess of the state MCL of 2 mg/L may get mottled teeth.

	TRICHLOROTRIFLUOROETHANE
	2025
	28
	N/A
	1200
	
	

	TRICHLOROFLUOROMETHANE
	2025
	12
	N/A
	150
	1300
	Discharge from industrial factories; degreasing solvent; propellant and


* While your drinking water meets the federal and state standard for arsenic, it does contain low levels of arsenic. The arsenic standard balances the current understanding of arsenic’s possible health effects against the costs of removing arsenic from drinking water. The U.S. Environmental Protection Agency continues to research the health effects of low levels of arsenic, which is a mineral known to cause cancer in humans at high concentrations and is linked to other health effects such as skin damage and circulatory problems.
** Nitrate in drinking water at levels above 10 mg/L is a health risk for infants of less than six months of age. Such nitrate levels in drinking water can interfere with the capacity of the infant’s blood to carry oxygen, resulting in a serious illness; symptoms include shortness of breath and blueness of the skin. Nitrate levels above 10 mg/L may also affect the ability of the blood to carry oxygen in other individuals, such as pregnant women and those with certain specific enzyme deficiencies. If you are caring for an infant, or you are pregnant, you should ask advice from your health care provider.

	TABLE 5 – DETECTION OF CONTAMINANTS WITH A SECONDARY DRINKING WATER STANDARD

	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
	PHG (MCLG)
	Typical Source of Contaminant

	Specific Conductance (EC) (µS/cm)
	2023
	240
	NA
	1,600
	N/A
	Substances that form ions when in water; seawater influence

	Sulfate (ppm)
	2023
	4
	NA
	500
	N/A
	Runoff/leaching from natural deposits; industrial wastes

	Total Dissolved Solids (TDS) (ppm)
	2023
	220
	NA
	1,000
	N/A
	Runoff/leaching from natural deposits

	Turbidity (NTU)
	2023
	0.33
	NA
	5
	N/A
	Soil runoff

	Chloride (ppm)
	2023
	5.2
	NA
	500
	N/A
	Runoff/leaching from natural deposits; seawater influence







	TABLE 6 – DETECTION OF UNREGULATED CONTAMINANTS

	Chemical or Constituent
(and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	Notification Level
	Health Effects Language

	Calcium (ppm)
	2023
	18
	NA
	N/A
	N/A

	Magnesium (ppm)
	2023
	10
	NA
	N/A
	N/A

	Potassium (ppm)
	2023
	5
	NA
	N/A
	N/A


The State allows us to monitor for some contaminants less than once per year because the concentrations of these contaminants do not change frequently. Some of our data, though representative, are more than one year old
Additional General Information on Drinking Water
Drinking water, including bottled water, may reasonably be expected to contain at least small amounts of some contaminants. The presence of contaminants does not necessarily indicate that the water poses a health risk. More information about contaminants and potential health effects can be obtained by calling the U.S. EPA’s Safe Drinking Water Hotline (1-800-426-4791).
Some people may be more vulnerable to contaminants in drinking water than the general population. Immuno-compromised persons such as persons with cancer undergoing chemotherapy, persons who have undergone organ transplants, people with HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections. These people should seek advice about drinking water from their health care providers. U.S. EPA/Centers for Disease Control (CDC) guidelines on appropriate means to lessen the risk of infection by Cryptosporidium and other microbial contaminants are available from the Safe Drinking Water Hotline (1-800-426-4791).
Lead-Specific Language: Lead can cause serious health problems, especially for pregnant women and young children. Lead in drinking water is primarily from materials and components associated with service lines and home plumbing. Countryside Care Center is responsible for providing high quality drinking water and removing lead pipes, but cannot control the variety of materials used in plumbing components in your home. You share the responsibility for protecting yourself and your family from the lead in your home plumbing. You can take responsibility by identifying and removing lead materials within your home plumbing and taking steps to reduce your family's risk. Before drinking tap water, flush your pipes for several minutes by running your tap, taking a shower, doing laundry or a load of dishes. You can also use a filter certified by an American National Standards Institute accredited certifier to reduce lead in drinking water. If you are concerned about lead in your water and wish to have your water tested, contact Superior Waterworks at 559-420-1534. Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available at http://www.epa.gov/safewater/lead.

Lead service line inventory has been prepared. Countryside Care Center water system was found to have no lead lines, fittings, or anything else containing lead. If you would like to have access to the inventory please email cotysuperiorwater@gmail.com and Superior Waterworks will send it over. 

For Water Systems Providing Groundwater as a Source of Drinking Water

	TABLE 7 – SAMPLING RESULTS SHOWING
FECAL INDICATOR-POSITIVE GROUNDWATER SOURCE SAMPLES

	Microbiological Contaminants
(complete if fecal-indicator detected)
	Total No. of Detections
	
Sample Dates
	MCL
[MRDL]
	PHG (MCLG) [MRDLG]
	
Typical Source of Contaminant

	E. coli
	0
	2024
	0
	(0)
	Human and animal fecal waste

	Enterococci
	0
	2024
	TT
	N/A
	Human and animal fecal waste

	Coliphage
	0
	2024
	TT
	N/A
	Human and animal fecal waste



