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[bookmark: _Toc58336712]2025 Consumer Confidence Report
[bookmark: _Toc58336713]Water System Information
Water System Name: Inyo County PWD – Lone Pine 
Report Date: June 16,2026
Type of Water Source(s) in Use: Groundwater Well
Name and General Location of Source(s): Wells 344 and 346 are located within the water service area of Lone Pine.
Drinking Water Source Assessment Information: The Source Water Assessment was completed in 2002 and is available by contacting Inyo County Public Works at (760) 878-0201.
Time and Place of Regularly Scheduled Board Meetings for Public Participation: Inyo County Board of Supervisors meeting schedule can be obtained at www.inyocounty.us
For More Information, Contact: Katie Paterson – (760) 878-8161
[bookmark: _Toc58336714]About This Report
We test the drinking water quality for many constituents as required by state and federal regulations.  This report shows the results of our monitoring for the period of January 1 to December 31, 2025, and may include earlier monitoring data.
Importance of This Report Statement in Five Non-English Languages (Spanish, Mandarin, Tagalog, Vietnamese, and Hmong)
Language in Spanish:  Este informe contiene información muy importante sobre su agua para beber.  Favor de comunicarse Inyo County PWD – Independence a (760) 878-8161 para asistirlo en español.
[bookmark: _Toc58336715]Terms Used in This Report
	Term
	Definition

	Level 1 Assessment
	A Level 1 assessment is a study of the water system to identify potential problems and determine (if possible) why total coliform bacteria have been found in our water system.

	Level 2 Assessment
	A Level 2 assessment is a very detailed study of the water system to identify potential problems and determine (if possible) why an E. coli MCL violation has occurred and/or why total coliform bacteria have been found in our water system on multiple occasions.

	Maximum Contaminant Level (MCL)
	The highest level of a contaminant that is allowed in drinking water.  Primary MCLs are set as close to the PHGs (or MCLGs) as is economically and technologically feasible.  Secondary MCLs are set to protect the odor, taste, and appearance of drinking water.

	Maximum Contaminant Level Goal (MCLG)
	The level of a contaminant in drinking water below which there is no known or expected risk to health.  MCLGs are set by the U.S. Environmental Protection Agency (U.S. EPA).

	Maximum Residual Disinfectant Level (MRDL)
	The highest level of a disinfectant allowed in drinking water.  There is convincing evidence that addition of a disinfectant is necessary for control of microbial contaminants.

	Maximum Residual Disinfectant Level Goal (MRDLG)
	The level of a drinking water disinfectant below which there is no known or expected risk to health.  MRDLGs do not reflect the benefits of the use of disinfectants to control microbial contaminants.

	Primary Drinking Water Standards (PDWS)
	MCLs and MRDLs for contaminants that affect health along with their monitoring and reporting requirements, and water treatment requirements.

	Public Health Goal
(PHG)
	The level of a contaminant in drinking water below which there is no known or expected risk to health.  PHGs are set by the California Environmental Protection Agency.

	Regulatory Action Level
(AL)
	The concentration of a contaminant which, if exceeded, triggers treatment or other requirements that a water system must follow.

	Secondary Drinking Water Standards (SDWS)
	MCLs for contaminants that affect taste, odor, or appearance of the drinking water.  Contaminants with SDWSs do not affect the health at the MCL levels.

	Treatment Technique
(TT)
	A required process intended to reduce the level of a contaminant in drinking water.

	Variances and Exemptions
	Permissions from the State Water Resources Control Board (State Board) to exceed an MCL or not comply with a treatment technique under certain conditions.

	ND
	Not detectable at testing limit.

	ppm
	parts per million or milligrams per liter (mg/L)

	ppb
	parts per billion or micrograms per liter (µg/L)

	ppt
	parts per trillion or nanograms per liter (ng/L)

	ppq
	parts per quadrillion or picogram per liter (pg/L)

	pCi/L
	picocuries per liter (a measure of radiation)


[bookmark: _Toc58336716]Sources of Drinking Water and Contaminants that May Be Present in Source Water
The sources of drinking water (both tap water and bottled water) include rivers, lakes, streams, ponds, reservoirs, springs, and wells.  As water travels over the surface of the land or through the ground, it dissolves naturally-occurring minerals and, in some cases, radioactive material, and can pick up substances resulting from the presence of animals or from human activity.
Contaminants that may be present in source water include:
Microbial contaminants, such as viruses and bacteria, that may come from sewage treatment plants, septic systems, agricultural livestock operations, and wildlife.
Inorganic contaminants, such as salts and metals, that can be naturally-occurring or result from urban stormwater runoff, industrial or domestic wastewater discharges, oil and gas production, mining, or farming.
Pesticides and herbicides, that may come from a variety of sources such as agriculture, urban stormwater runoff, and residential uses.
Organic chemical contaminants, including synthetic and volatile organic chemicals, that are byproducts of industrial processes and petroleum production, and can also come from gas stations, urban stormwater runoff, agricultural application, and septic systems.
Radioactive contaminants, that can be naturally-occurring or be the result of oil and gas production and mining activities.
Regulation of Drinking Water and Bottled Water Quality
In order to ensure that tap water is safe to drink, the U.S. EPA and the State Board prescribe regulations that limit the amount of certain contaminants in water provided by public water systems.  The U.S. Food and Drug Administration regulations and California law also establish limits for contaminants in bottled water that provide the same protection for public health.
[bookmark: _Toc58336717]About Your Drinking Water Quality
[bookmark: _Toc58336718][bookmark: _Hlk57994699]Drinking Water Contaminants Detected
Tables 1, 2, 3, 4, 5, 6, and 8 list all of the drinking water contaminants that were detected during the most recent sampling for the constituent.  The presence of these contaminants in the water does not necessarily indicate that the water poses a health risk.  The State Board allows us to monitor for certain contaminants less than once per year because the concentrations of these contaminants do not change frequently.  Some of the data, though representative of the water quality, are more than one year old.  Any violation of an AL, MCL, MRDL, or TT is asterisked.  Additional information regarding the violation is provided later in this report.
Table 1.  Sampling Results Showing the Detection of Coliform Bacteria
Complete if bacteria are detected.

	Microbiological Contaminants 
	Highest No. of Detections
	No. of Months in Violation
	MCL
	MCLG
	Typical Source of Bacteria

	E. coli

	(In the year)
0
	0
	(a)
	0
	Human and animal fecal waste



(a) Routine and repeat samples are total coliform-positive and either is E. coli-positive or system fails to take repeat samples following E. coli-positive routine sample or system fails to analyze total coliform-positive repeat sample for E. coli.
Table 2.  Sampling Results Showing the Detection of Lead and Copper
Complete if lead or copper is detected in the last sample set.

	Lead and Copper 
	Sample Date
	No. of Samples Collected
	90th Percentile Level Detected
	No. Sites Exceeding AL
	Range of Results
	AL
	PHG
	Typical Source of
Contaminant

	Lead (ppb)
	9-12-25
	10
	0
	0
	ND
	15
	0.2
	Corrosion of household plumbing systems; Erosion of natural deposits

	Copper (ppm)
	9-12-25
	10
	0.48
	0
	0 – 0.53
	1.3
	0.3
	Internal corrosion of household plumbing systems; erosion of natural deposits; leaching from wood preservatives


Table 3.  Sampling Results for Sodium and Hardness
	Chemical or Constituent (and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
	PHG (MCLG)
	Typical Source of Contaminant

	Sodium (ppm)
	5-3-2023
	21.55
	15.6 – 27.5
	None
	None
	Salt present in the water and is generally naturally occurring

	Hardness (ppm)
	5-3-2023
	72.25
	72.2 – 72.3
	None
	None
	Sum of polyvalent cations present in the water, generally magnesium and calcium, and are usually naturally occurring


Table 4.  Detection of Contaminants with a Primary Drinking Water Standard
	Chemical or Constituent
(and
reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL [MRDL]
	PHG (MCLG) [MRDLG]
	Typical Source of Contaminant

	Gross Alpha (pCi/L)
	8-12-2020
	4.5
	4.0 – 5.0
	15
	0
	Erosion of natural deposits.

	Uranium (pCi/L)
	6-12-2017
	3.29
	2.35 – 4.22
	20
	0.43
	Erosion of natural deposits.

	Arsenic (ppb)
	5-3-2023
	ND
	N/A
	10
	0.004
	Erosion of natural deposits; runoff from orchards; glass and electronics production wastes.

	Barium (mg/L)
	5-3-2023
	11.35
	10.6 – 12.1
	1
	2
	Discharges of oil drilling wastes and from metal refineries; erosion of natural deposits.

	Copper (mg/L)
	5-3-2023
	15.95
	3.7 – 28.2
	1
	0.3
	Internal corrosion of household plumbing systems; erosion of natural deposits; leaching from wood preservatives.

	Fluoride (mg/L)
	5-3-2023
	ND
	N/A
	2.0
	1
	Erosion of natural deposits; water additive that promotes strong teeth; discharge from fertilizer and aluminum factories.

	Nitrate (mg/L)
	5-13-2025
	0.287
	0.221 – 0.353
	10
	10
	Runoff and leaching from fertilizer use; leaching from septic tanks and sewage; erosion of natural deposits.

	Perchlorate (ppb)
	5-3-2023
	ND
	N/A
	6
	1
	Perchlorate is an inorganic chemical used in solid rocket propellant, fireworks, explosives, flares, matches, and a variety of industries. It usually gets into drinking water as a result of environmental contamination from historic aerospace or other industrial operations that used or use, store, or dispose of perchlorate and its salts.

	Combined Radium (pCi/L)
	6-12-2017
	ND
	N/A
	5
	0
	Erosion of natural deposits.

	Chromium (hexavalent) (ug/L)
	12-17-2024
	0.323
	0 – 0.323
	10
	0.02
	Erosion of natural deposits; transformation of naturally occurring trivalent chromium to hexavalent chromium by natural processes and human activities such as discharges from electroplating factories, leather tanneries, wood preservation, chemical synthesis, refractory production, and textile manufacturing facilities.

	Chlorine (mg/L)
	2025
	0
	N/A
	4
	4
	Drinking water disinfectant added for treatment.

	TTHMs (Total Trihalomethanes) (ug/L)
	12-29-2025
	ND
	N/A
	80
	N/A
	Byproduct of drinking water disinfection.

	HAA5 (Sum of 5 Haloacetic Acids) (ug/L)
	12-29-2025
	ND
	N/A
	60
	N/A
	Byproduct of drinking water disinfection.


Table 5.  Detection of Contaminants with a Secondary Drinking Water Standard
	Chemical or Constituent (and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	SMCL
	PHG (MCLG)
	Typical Source
of
Contaminant

	Color (Units)
	5-3-2023
	5
	4 – 5
	15
	N/A
	Naturally occurring organic materials.

	Turbidity (NTU)
	10-21-2025
	1.45
	1.25 – 1.65
	5
	N/A
	Soil runoff.

	Total Dissolved Solids (ppm)
	5-3-2023
	150
	125 – 174
	1,000
	N/A
	Runoff/leaching from natural deposits.

	Specific Conductance (uS/cm)
	10-21-2025
	211
	209.0 – 212.6
	1,600
	N/A
	Substances that form when in water.

	Chloride (ppm)
	5-3-2023
	10.8
	9.01 – 12.4
	500
	N/A
	Runoff/leaching from natural deposits.

	Sulfate (ppm)
	5-3-2023
	15.85
	13.2 – 18.5
	500
	N/A
	Runoff/leaching from natural deposits.


Table 6.  Detection of Unregulated Contaminants
	Chemical or Constituent (and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	Notification Level
	Health Effects 

	Boron (mg/L)
	5-3-2023
	234.5
	116 – 353
	1
	Boron exposures resulted in decreased fetal weight (developmental effects) in newborn rats.

	Radon (pCi/L)
	5-1-2012
	200.00
	N/A
	N/A
	See below.


[bookmark: _Toc58336719]Additional General Information on Drinking Water
Drinking water, including bottled water, may reasonably be expected to contain at least small amounts of some contaminants.  The presence of contaminants does not necessarily indicate that the water poses a health risk.  More information about contaminants and potential health effects can be obtained by calling the U.S. EPA’s Safe Drinking Water Hotline (1-800-426-4791).
Some people may be more vulnerable to contaminants in drinking water than the general population.  Immuno-compromised persons such as persons with cancer undergoing chemotherapy, persons who have undergone organ transplants, people with HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections.  These people should seek advice about drinking water from their health care providers.  U.S. EPA/Centers for Disease Control (CDC) guidelines on appropriate means to lessen the risk of infection by Cryptosporidium and other microbial contaminants are available from the Safe Drinking Water Hotline (1-800-426-4791).
Lead-Specific Language: Lead can cause serious health problems, especially for pregnant women and young children. Lead in drinking water is primarily from materials and components associated with service lines and home plumbing. Inyo County PWD – Laws Town is responsible for providing high quality drinking water and removing lead pipes, but cannot control the variety of materials used in plumbing components in your home. You share the responsibility for protecting yourself and your family from the lead in your home plumbing. You can take responsibility by identifying and removing lead materials within your home plumbing and taking steps to reduce your family's risk. Before drinking tap water, flush your pipes for several minutes by running your tap, taking a shower, doing laundry or a load of dishes. You can also use a filter certified by an American National Standards Institute accredited certifier to reduce lead in drinking water. If you are concerned about lead in your water and wish to have your water tested, contact Inyo County PWD – Laws Town at (760) 878-8161. Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available at http://www.epa.gov/safewater/lead.

Additional Special Language for Nitrate, Arsenic, Lead, Radon, and Cryptosporidium: We constantly monitor the water supply for various contaminants. We have consistently detected radon in the groundwater supply. There is no federal regulation for radon levels in drinking water. Exposure over a long period of time to air transmitting radon may cause adverse health effects. Radon is radioactive gas that you cannot see, taste or smell. It is found throughout the U.S. Radon can move up through the ground and into a home through cracks and holes in the foundation. Radon can build up to high levels in all types of homes. Radon can also get into indoor air when released from tap water from showering, washing dishes, and other household activities. Compared to radon entering the home through soil, radon entering the home through tap water will in most cases be a small source of radon in indoor air. Radon is a known human carcinogen. Breathing air containing radon can lead to lung cancer. Drinking water containing radon may also cause increased risk of stomach cancer. If you are concerned about radon in your home, test the air in your home. Testing is inexpensive and easy. You should pursue radon removal for your home if the level of radon in your air is 4 picocuries per liter of air (pCi/L) or higher. There are simple and inexpensive ways to fix a radon problem. For additional information, call your state radon program (1-800-745-7236), the U.S. EPA Safe Drinking Water Act Hotline (1-800-426-4791), or the National Safe Council Radon Hotline (1-800-767-7236.) State Revised Total Coliform Rule (RTCR): [Enter Additional Information Described in Instructions for SWS CCR Document]
[bookmark: _Toc58336720]Summary Information for Violation of a MCL, MRDL, AL, TT, or Monitoring and Reporting Requirement
Table 7. Violation of a MCL, MRDL, AL, TT or Monitoring Reporting Requirement
	Violation
	Explanation
	Duration
	Actions Taken to Correct Violation
	Health Effects Language

	Failure to submit lead line service inventory.
	Failed to submit lead line service inventory.
	2025 -2026
	Submit the lead line service inventory.
	Infants and children who drink water containing lead in excess of the action level may experience delays in their physical or mental development. Children may show slight deficits in attention span and learning abilities. Adults who drink this water over many years may develop kidney problems or high blood pressure. Copper is an essential nutrient, but some people who drink water containing copper in excess of the action level over a relatively short amount of time may experience gastrointestinal distress. Some people who drink water containing copper in excess of the action level over many years may suffer liver or kidney damage. People with Wilson’s Disease should consult their personal doctor.   

	Failure to monitor for Disinfection Byproducts
	Failed to collect Disinfection Byproduct samples
	2025
	Samples will be collected.
	Some people who drink water containing trihalomethanes in excess of the MCL over many years may experience liver, kidney, or central nervous system problems, and may have an increased risk of getting cancer. Some people who drink water containing haloacetic acids in excess of MCL over many years may have an increased risk of getting cancer.



[bookmark: _Toc58336721]For Water Systems Providing Groundwater as a Source of Drinking Water
Table 8.  Sampling Results Showing Fecal Indicator-Positive Groundwater Source Samples
	Microbiological Contaminants (complete if fecal-indicator detected)
	Total No. of Detections
	Sample Dates
	MCL [MRDL]
	PHG (MCLG) [MRDLG]
	Typical Source of Contaminant

	E. coli
	(In the year)
0
	2025
	0
	(0)
	Human and animal fecal waste

	Enterococci
	(In the year)
0
	2025
	TT
	N/A
	Human and animal fecal waste

	Coliphage
	(In the year)
0
	2025
	TT
	N/A
	Human and animal fecal waste
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