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[bookmark: _Toc58336712]2022 Consumer Confidence Report
[bookmark: _Toc58336713]Water System Information
Water System Name: Rod McLellan Botanicals WS 
Report Date: June 29, 2023
Type of Water Source(s) in Use: Groundwater 
Name and General Location of Source(s): Well #1 and Well # 2 (standby) are located at Taisuco America Corporation’s Corporate Office site of 2352 San Juan Road, Aromas CA 95004. Well # 1 is just below the main office building and well # 2 is about 100 meters South-East of that. 
Drinking Water Source Assessment Information:  On a monthly basis before taking the routine bacteria samples for Total Coliform & E. coli, the distribution system, wells and holding tanks are reviewed for leaks and any possible issues. The numerous valves in the inspection route are exercised and checked for deficiencies. Meters are read and recorded on a monthly basis. Maintenance of the system is done on an as-needed basis. The holding tank A is flushed quarterly for a short interval to remove possible debris that settles to the bottom of the tank. Disinfection is done annually or if a Positive bacteria sample in the well or tank.  
Time and Place of Regularly Scheduled Board Meetings for Public Participation: This is a Private Business System and thus no public participation. 
For More Information, Contact: System Operator Richard Muñoz, License # (28771) at 831-726-1797 Ext. 107 Office or Cell # 831-234-4112 for 24/7 service. 
[bookmark: _Toc58336714]About This Report
We test the drinking water quality for many constituents as required by state and federal regulations.  This report shows the results of our monitoring for the period of January 1 to December 31, 2022 and may include earlier monitoring data.
Importance of This Report Statement in Five Non-English Languages (Spanish, Mandarin, Tagalog, Vietnamese, and Hmong)
Language in Spanish:  Este informe contiene información muy importante sobre su agua para beber.  Favor de comunicarse Rod McLellan Botanicals WS a 2352 San Juan Road, Aromas CA 95004, 831-726-1797 para asistirlo en español.
Language in Mandarin:  这份报告含有关于您的饮用水的重要讯息。请用以下地址和电话联系 Rod McLellan Botanicals WS以获得中文的帮助: 2352 San Juan Road, Aromas, CA 95004, 831-726-1797
Language in Tagalog: Ang pag-uulat na ito ay naglalaman ng mahalagang impormasyon tungkol sa inyong inuming tubig.  Mangyaring makipag-ugnayan sa Rod McLellan Botanicals WS, 2352 San Juan Road, Aromas CA 95004 o tumawag sa 831-726-1797 para matulungan sa wikang Tagalog.
Language in Vietnamese:  Báo cáo này chứa thông tin quan trọng về nước uống của bạn.  Xin vui lòng liên hệ Rod McLellan Botanicals WS tại 2352 San Juan Road, Aromas CA 95004, 831-726-1797 để được hỗ trợ giúp bằng tiếng Việt.
Language in Hmong:  Tsab ntawv no muaj cov ntsiab lus tseem ceeb txog koj cov dej haus.  Thov hu rau Rod McLellan Botanicals WS ntawm 2352 San Juan Road, Aromas CA 95004, 831-726-1797 rau kev pab hauv lus Askiv.
[bookmark: _Toc58336715]Terms Used in This Report
	Term
	Definition

	Level 1 Assessment
	A Level 1 assessment is a study of the water system to identify potential problems and determine (if possible) why total coliform bacteria have been found in our water system.

	Level 2 Assessment
	A Level 2 assessment is a very detailed study of the water system to identify potential problems and determine (if possible) why an E. coli MCL violation has occurred and/or why total coliform bacteria have been found in our water system on multiple occasions.

	Maximum Contaminant Level (MCL)
	The highest level of a contaminant that is allowed in drinking water.  Primary MCLs are set as close to the PHGs (or MCLGs) as is economically and technologically feasible.  Secondary MCLs are set to protect the odor, taste, and appearance of drinking water.

	Maximum Contaminant Level Goal (MCLG)
	The level of a contaminant in drinking water below which there is no known or expected risk to health.  MCLGs are set by the U.S. Environmental Protection Agency (U.S. EPA).

	Maximum Residual Disinfectant Level (MRDL)
	The highest level of a disinfectant allowed in drinking water.  There is convincing evidence that addition of a disinfectant is necessary for control of microbial contaminants.

	Maximum Residual Disinfectant Level Goal (MRDLG)
	The level of a drinking water disinfectant below which there is no known or expected risk to health.  MRDLGs do not reflect the benefits of the use of disinfectants to control microbial contaminants.

	Primary Drinking Water Standards (PDWS)
	MCLs and MRDLs for contaminants that affect health along with their monitoring and reporting requirements, and water treatment requirements.

	Public Health Goal
(PHG)
	The level of a contaminant in drinking water below which there is no known or expected risk to health.  PHGs are set by the California Environmental Protection Agency.

	Regulatory Action Level
(AL)
	The concentration of a contaminant which, if exceeded, triggers treatment or other requirements that a water system must follow.

	Secondary Drinking Water Standards (SDWS)
	MCLs for contaminants that affect taste, odor, or appearance of the drinking water.  Contaminants with SDWSs do not affect the health at the MCL levels.

	Treatment Technique
(TT)
	A required process intended to reduce the level of a contaminant in drinking water.

	Variances and Exemptions
	Permissions from the State Water Resources Control Board (State Board) to exceed an MCL or not comply with a treatment technique under certain conditions.

	ND
	Not detectable at testing limit.

	ppm
	parts per million or milligrams per liter (mg/L)

	ppb
	parts per billion or micrograms per liter (µg/L)

	ppt
	parts per trillion or nanograms per liter (ng/L)

	ppq
	parts per quadrillion or picogram per liter (pg/L)

	pCi/L
	picocuries per liter (a measure of radiation)


[bookmark: _Toc58336716]Sources of Drinking Water and Contaminants that May Be Present in Source Water
The sources of drinking water (both tap water and bottled water) include rivers, lakes, streams, ponds, reservoirs, springs, and wells.  As water travels over the surface of the land or through the ground, it dissolves naturally-occurring minerals and, in some cases, radioactive material, and can pick up substances resulting from the presence of animals or from human activity.
Contaminants that may be present in source water include:
Microbial contaminants, such as viruses and bacteria, that may come from sewage treatment plants, septic systems, agricultural livestock operations, and wildlife.
Inorganic contaminants, such as salts and metals, that can be naturally-occurring or result from urban stormwater runoff, industrial or domestic wastewater discharges, oil and gas production, mining, or farming.
Pesticides and herbicides, that may come from a variety of sources such as agriculture, urban stormwater runoff, and residential uses.
Organic chemical contaminants, including synthetic and volatile organic chemicals, that are byproducts of industrial processes and petroleum production, and can also come from gas stations, urban stormwater runoff, agricultural application, and septic systems.
Radioactive contaminants, that can be naturally-occurring or be the result of oil and gas production and mining activities.
Regulation of Drinking Water and Bottled Water Quality
In order to ensure that tap water is safe to drink, the U.S. EPA and the State Board prescribe regulations that limit the amount of certain contaminants in water provided by public water systems.  The U.S. Food and Drug Administration regulations and California law also establish limits for contaminants in bottled water that provide the same protection for public health.
[bookmark: _Toc58336717]About Your Drinking Water Quality
[bookmark: _Toc58336718][bookmark: _Hlk57994699]Drinking Water Contaminants Detected
Tables 1, 2, 3, 4, 5, 6, and 8 list all of the drinking water contaminants that were detected during the most recent sampling for the constituent.  The presence of these contaminants in the water does not necessarily indicate that the water poses a health risk.  The State Board allows us to monitor for certain contaminants less than once per year because the concentrations of these contaminants do not change frequently.  Some of the data, though representative of the water quality, are more than one year old.  Any violation of an AL, MCL, MRDL, or TT is asterisked.  Additional information regarding the violation is provided later in this report.
Table 1.  Sampling Results Showing the Detection of Coliform Bacteria
Complete if bacteria are detected.

	Microbiological Contaminants 
	Highest No. of Detections
	No. of Months in Violation
	MCL
	MCLG
	Typical Source of Bacteria

	E. coli

	(0)

	0
	( see a below)
	0
	Human and animal fecal waste



(a) Routine and repeat samples are total coliform-positive and either is E. coli-positive or system fails to take repeat samples following E. coli-positive routine sample or system fails to analyze total coliform-positive repeat sample for E. coli.
Table 2.  Sampling Results Showing the Detection of Lead and Copper
Complete if lead or copper is detected in the last sample set.

	Lead and Copper 
	Sample Date
	No. of Samples Collected
	90th Percentile Level Detected
	No. Sites Exceeding AL
	AL
	PHG
	Typical Source of
Contaminant

	Lead (ppb)
	6/14/2021
	8
	ND
	0
	15
	0.2
	Internal corrosion of household water plumbing systems; discharges from industrial manufacturers; erosion of natural deposits

	Copper (ppm)
	[bookmark: _GoBack]6/14/2021
	8
	0.295
	0
	1.3
	0.3
	Internal corrosion of household plumbing systems; erosion of natural deposits; leaching from wood preservatives


Table 3.  Sampling Results for Sodium and Hardness
	Chemical or Constituent (and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL
	PHG (MCLG)
	Typical Source of Contaminant

	Sodium (ppm)
	4/28/2021
	72
	1
	None
	None
	Salt present in the water and is generally naturally occurring

	Hardness (ppm)
	4/28/2021
	264
	5
	None
	None
	Sum of polyvalent cations present in the water, generally magnesium and calcium, and are usually naturally occurring


Table 4.  Detection of Contaminants with a Primary Drinking Water Standard
	Chemical or Constituent
(and
reporting units)
	Sample Date
	Level Detected
	Range of Detections
	MCL [MRDL]
	PHG (MCLG) [MRDLG]
	Typical Source of Contaminant

	Turbidity NTU
	4/28/2021
	0.10
	0.1
	5
	N/A
	Soil runoff

	Gross Alpha
Particle Activity
pCi/L
	5/18/2021
	5.00 +-
0.793
	N/A
	15
	0
	Erosion of natural deposits

	Strontium Total
Ug/L
	4/28/2021
	483
	2
	None
	N/A
	Decay of natural and man-made deposits

	Arsenic
Ug/L
	4/28/2021
	2.2
	1
	10
	0.004
	Erosion of natural deposits; glass and electronics

	Barium
Ug/L
	4/28/2021
	110
	5
	1000
	2
	Discharge of oil drilling waste and from metal refineries; erosion of natural deposits

	



Chromium Total
Ug/L
	



4/28/2021
	



3.4
	



1
	



50
	



100
	


Discharge from steel and pulp mills and chrome plating; erosion of natural deposits

	Nickel 
Ug/L
	4/28/2021
	10.1
	5
	100
	12
	Erosion of natural deposits; discharge from metal factories

	Nitrate 
Nitrogen, N
Mg/L
	12/13/2022
	9.2
	0.1
	10
	10
	Runoff and leaching from fertilizer use; leaching from septic tanks and sewage; erosion of natural deposits

	Selenium
Ug/L
	4/28/2021
	6.7
	1
	50
	30
	Discharge from petroleum, glass and metal refineries; erosion of natural deposits; discharge from mines and chemicals manufacturers; runoff from livestock lots (feed additive).


Table 5.  Detection of Contaminants with a Secondary Drinking Water Standard
	Chemical or Constituent (and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	SMCL
	PHG (MCLG)
	Typical Source
of
Contaminant

	Turbidity 
Ug/L
	4/28/2021
	0.10
	0.1
	5
	N/A
	Soil runoff 

	Zinc 
Mg/L
	4/28/2021
	0.03
	0.03
	5
	N/A
	Runoff/leaching from natural deposits; industrial waste.

	* Total Dissolved Solids (TDS)
	5/31/2022
	552
	0.01
	500
	N/A
	Runoff/leaching from natural deposits. 

	* Specific Conductance
umhos/cm 
	4/28/2021
	911
	3
	900
	N/A
	Substances that from ions when in water; seawater influence

	Chlorine 
mg/L
	4/28/2021
	0.162
	0.001
	0.25
	N/A
	Runoff/leaching from natural deposits; seawater influence 

	Sulfate
mg/L
	4/28/2021
	0.041
	0.001
	0.25
	N/A
	Runoff/leaching from natural deposits; industrial waste


Table 6.  Detection of Unregulated Contaminants
	Chemical or Constituent (and reporting units)
	Sample Date
	Level Detected
	Range of Detections
	Notification Level
	Health Effects 

	Silica (Sio2), Total 
mg/L
	4/28/2021
	46.1
	1
	N/A
	N/A

	Calcium
mg/L
	4/28/2021
	63
	1
	N/A
	N/A

	Magnesium
mg/L
	4/28/2021
	25.6
	0.5
	N/A
	N/A

	Potassium
mg/L
	4/28/2021
	1.6
	0.5
	N/A
	N/A

	Alkalinity, Total 
(as CaC03)
mg/L
	4/28/2021
	123
	10
	N/A
	N/A

	Bicarbonate 
(as HC03)
mg/L
	4/28/2021
	150
	10
	N/A
	N/A

	pH
pH (H)
	4/28/2021
	6.5
	0.1
	8.5
	N/A


[bookmark: _Toc58336719]Additional General Information on Drinking Water
Drinking water, including bottled water, may reasonably be expected to contain at least small amounts of some contaminants.  The presence of contaminants does not necessarily indicate that the water poses a health risk.  More information about contaminants and potential health effects can be obtained by calling the U.S. EPA’s Safe Drinking Water Hotline (1-800-426-4791).
Some people may be more vulnerable to contaminants in drinking water than the general population.  Immuno-compromised persons such as persons with cancer undergoing chemotherapy, persons who have undergone organ transplants, people with HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections.  These people should seek advice about drinking water from their health care providers.  U.S. EPA/Centers for Disease Control (CDC) guidelines on appropriate means to lessen the risk of infection by Cryptosporidium and other microbial contaminants are available from the Safe Drinking Water Hotline (1-800-426-4791).
Lead-Specific Language:  If present, elevated levels of lead can cause serious health problems, especially for pregnant women and young children.  Lead in drinking water is primarily from materials and components associated with service lines and home plumbing.  Rod McLellan Botanicals WS is responsible for providing high quality drinking water but cannot control the variety of materials used in plumbing components.  When your water has been sitting for several hours, you can minimize the potential for lead exposure by flushing your tap for 30 seconds to 2 minutes before using water for drinking or cooking.  [Optional: If you do so, you may wish to collect the flushed water and reuse it for another beneficial purpose, such as watering plants.]  If you are concerned about lead in your water, you may wish to have your water tested.  Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available from the Safe Drinking Water Hotline (1-800-426-4791) or at http://www.epa.gov/lead.
Radon – Radon is a radioactive gas that you cannot see, taste, or smell.  It is found throughout the U.S.  Radon can move up through the ground and into a home through cracks and holes in the foundation.  Radon can build up to high levels in all types of homes.  Radon can also get into indoor air when released from tap water from showering, washing dishes, and other household activities.  Compared to radon entering the home through soil, radon entering the home through tap water will in most cases be a small source of radon in indoor air.  Radon is a known human carcinogen.  Breathing air containing radon can lead to lung cancer.  Drinking water containing radon may also cause increased risk of stomach cancer.  If you are concerned about radon in your home, test the air in your home.  Testing is inexpensive and easy.  You should pursue radon removal for your home if the level of radon in your air is 4 picocuries per liter of air (pCi/L) or higher.  There are simple ways to fix a radon problem that are not too costly.  For additional information, call your State radon program (1-800-745-7236), the U.S. EPA Safe Drinking Water Hotline (1-800-426-4791), or the National Safety Council Radon Hotline (1‑800-767-7236).
	 Arsenic - While your drinking water meets the federal and state standard for arsenic, it does contain low levels of arsenic.  The arsenic standard balances the current understanding of arsenic’s possible health effects against the costs of removing arsenic from drinking water.  The U.S. Environmental Protection Agency continues to research the health effects of low levels of arsenic, which is a mineral known to cause cancer in humans at high concentrations and is linked to other health effects such as skin damage and circulatory problems.



Additional Special Language for Nitrate, Arsenic, Lead, Radon, and Cryptosporidium: Nitrate in drinking water at levels above 10 mg/L is a health risk for infants of less than six months of age.  Such nitrate levels in drinking water can interfere with the capacity of the infant’s blood to carry oxygen, resulting in serious illness; symptoms include shortness of breath and blueness of the skin.  Nitrate levels above 10 mg/L may also affect the ability of the blood to carry oxygen in other individuals, such as pregnant women and those with specific enzyme deficiencies.  If you are caring for an infant, or you are pregnant, you should ask advice from your health care provider.

State Revised Total Coliform Rule (RTCR): Level 1 Assessment
	If a water system collects...
	Level 1 Assessment is required within 30 days if...

	...Less than 40 routine and repeat samples per month
	More than 1 TC-positive sample in a month

	...40 or more routine and repeat samples per month
	More than 5.0% TC-positive samples in a month

	…a sample that is total coliform positive
	Fails to collect all required repeat samples


Under the RTCR, a water system which exceeds one of the trigger levels in the table above must conduct a Level 1 Assessment within 30 days. The completed assessment must be submitted to the local regulating agency (DDW District Office or County Health Office) within 30 days of exceeding the trigger level. The Level 1 Assessment will require water systems to identify a possible cause to the total coliform positive samples and corrective actions taken/needed. Failure to conduct or submit a completed assessment, or failure to complete the corrective actions is a violation of the Coliform Treatment Technique in the RTCR. Water system will follow the established Sample Site Plan registered with their Primacy for Repeat Samples. 
 
[bookmark: _Toc58336720]Summary Information for Violation of a MCL, MRDL, AL, TT, or Monitoring and Reporting Requirement
Table 7. Violation of a MCL, MRDL, AL, TT or Monitoring Reporting Requirement
	Violation
	Explanation
	Duration
	Actions Taken to Correct Violation
	Health Effects Language

	None
	N/A
	N/A
	N/A
	N/A

	
	
	
	
	



[bookmark: _Toc58336721]For Water Systems Providing Groundwater as a Source of Drinking Water
Table 8.  Sampling Results Showing Fecal Indicator-Positive Groundwater Source Samples
	Microbiological Contaminants (complete if fecal-indicator detected)
	Total No. of Detections
	Sample Dates
	MCL [MRDL]
	PHG (MCLG) [MRDLG]
	Typical Source of Contaminant

	E. coli
	0
	N/A
	0
	(0)
	Human and animal fecal waste

	Enterococci
	0
	N/A
	TT
	N/A
	Human and animal fecal waste

	Coliphage
	(In the year)
[Enter No.]
	[Enter Dates]
	TT
	N/A
	Human and animal fecal waste


[bookmark: _Toc58336722]Summary Information for Fecal Indicator-Positive Groundwater Source Samples, Uncorrected Significant Deficiencies, or Violation of a Groundwater TT
	Special Notice of Fecal Indicator-Positive Groundwater Source Sample: Rod McLellan Botanicals WS did not have any Fecal Positive Indicators 



	Special Notice for Uncorrected Significant Deficiencies: Rod McLellan Botanicals WS did not have any uncorrected significant Deficiencies with its water system. 



Table 9. Violation of Groundwater TT
	Violation
	Explanation
	Duration
	Actions Taken to Correct Violation
	Health Effects Language

	None
	N/A
	N/A
	N/A
	N/A

	
	
	
	
	


[bookmark: _Toc58336725][bookmark: _Hlk58234306]Summary Information for Operating Under a Variance or Exemption
Rod McLellan Botanicals Water System did not operate under a Variance or Exemption. 
Note: The information below is left in for employee informational purposes only. 
Rod McLellan Botanicals Water System did not have a Level 1 or Level 2 Assessment requirement. The water system did not have any sanitary defects. The water system does not have treatment or needed to do treatment because of a violation or exceedance of the MCL. The system also did not have any Total Coliform or E. Coli Present samples. 
[bookmark: _Toc58336726]Summary Information for Revised Total Coliform Rule Level 1 and Level 2 Assessment Requirements
If a water system is required to comply with a Level 1 or Level 2 assessment requirement that is not due to an E. coli MCL violation, include the following information below [22 CCR section 64481(n)(1)].

Level 1 or Level 2 Assessment Requirement not Due to an E. coli MCL Violation
Coliforms are bacteria that are naturally present in the environment and are used as an indicator that other, potentially harmful, waterborne pathogens may be present or that a potential pathway exists through which contamination may enter the drinking water distribution system.  We found coliforms indicating the need to look for potential problems in water treatment or distribution.  When this occurs, we are required to conduct assessment(s) to identify problems and to correct any problems that were found during these assessments.
The water system shall include the following statements, as appropriate:
[bookmark: _Hlk534984154][bookmark: _Hlk534984203]During the past year we were required to conduct [Insert Number of Level 1 Assessments] Level 1 assessment(s).  [Insert Number of Level 1 Assessments] Level 1 assessment(s) were completed.  In addition, we were required to take [Insert Number of Corrective Actions] corrective actions and we completed [Insert Number of Corrective Actions] of these actions.
[bookmark: _Hlk535238544][bookmark: _Hlk535238579]During the past year [Insert Number of Level 2 Assessment] Level 2 assessments were required to be completed for our water system.  [Insert Number of Level 2 Assessments] Level 2 assessments were completed.  In addition, we were required to take [Insert Number of Corrective Actions] corrective actions and we completed [Insert Number of Corrective Actions] of these actions.
If the water system failed to complete all the required assessments or correct all identified sanitary defects, the water system is in violation of the treatment technique requirement and shall include the following statements, as appropriate:
During the past year we failed to conduct all of the required assessment(s).

During the past we failed to correct all identified defects that were found during the assessment.

[For Violation of the Total Coliform Bacteria TT Requirement, Enter Additional Information Described in Instructions for SWS CCR Document]
If a water system is required to comply with a Level 2 assessment requirement that is due to an E. coli MCL violation, include the information below [22 CCR section 64481(n)(2)].
Level 2 Assessment Requirement Due to an E. coli MCL Violation
E. coli are bacteria whose presence indicates that the water may be contaminated with human or animal wastes.  Human pathogens in these wastes can cause short-term effects, such as diarrhea, cramps, nausea, headaches, or other symptoms.  They may pose a greater health risk for infants, young children, the elderly, and people with severely compromised immune systems.  We found E. coli bacteria, indicating the need to look for potential problems in water treatment or distribution.  When this occurs, we are required to conduct assessment(s) identify problems and to correct any problems that were found during these assessments.
We were required to complete a Level 2 assessment because we found E. coli in our water system.  In addition, we were required to take [Insert Number of Corrective Actions] corrective actions and we completed [Insert Number of Corrective Actions] of these actions.
If a water system failed to complete the required assessment or correct all identified sanitary defects, the water system is in violation of the treatment technique requirement and shall include the following statements, as appropriate:
We failed to conduct the required assessment.

We failed to correct all sanitary defects that were identified during the assessment.

If a water system detects E. coli and has violated the E. coli MCL, include one or more the following statements to describe any noncompliance, as applicable: 
We had an E. coli-positive repeat sample following a total coliform positive routine sample.

We had a total coliform-positive repeat sample following an E. coli-positive routine sample.

We failed to take all required repeat samples following an E. coli-positive routine sample.

We failed to test for E. coli when any repeat sample tests positive for total coliform.

[If a water system detects E. coli and has not violated the E. coli MCL, the water system may include a statement that explains that although they have detected E. coli, they are not in violation of the E. coli MCL.]
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