{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["WQ Report","Lab Data"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"WQ Report","index":0,"n_rows":147,"n_cols":7,"rows_kept":147,"cut":false,"hidden":false,"merged":[[94,7,94,11],[95,7,95,11],[89,7,89,11],[90,7,90,11],[24,0,24,6],[51,0,51,6],[146,0,146,6],[105,0,105,6],[88,0,88,6],[93,0,93,6],[91,0,91,6],[130,0,130,6],[141,0,141,6]]}
["Parameter","Units","Year \nTested","MCL","DLR","Chino I\nDesalter","Comments"]
["Parameter","Units","Year \nTested","MCL","DLR","Chino I\nDesalter","Comments"]
["PRIMARY  STANDARDS - Mandatory Health-Related Standards"]
["Inorganic Chemicals (IOCs)",null,null,null,null,null,"Storet #"]
["Aluminum","ppb",2020,1000,50,"< 50","01105"]
["Antimony","ppb",2020,6,6,"< 6","01097"]
["Arsenic","ppb",2020,10,2,"< 2","01002"]
["Asbestos","MFL",2020,7,0.2,0,"81855"]
["Barium","ppb",2020,1000,100,"< 100","01007"]
["Beryllium","ppb",2020,4,1,"< 1","01012"]
["Cadmium","ppb",2020,5,1,"< 1","01027"]
["Total Chromium","ppb",2020,50,10,"< 10","01034"]
["Copper","ppb",2020,1000,50,"< 50","01042"]
["Cyanide","ppb",2020,150,100,"< 100","01291"]
["Fluoride","ppm",2020,2,0.1,"< 0.1","00951"]
["Hexavalent Chromium","ppb",2020,10,1,"< 1","01032"]
["Lead","ppb",2020,15,5,"< 5","01051"]
["Mercury","ppb",2020,2,1,"< 1","71900"]
["Nickel","ppb",2020,100,10,"< 10","01067"]
["Nitrate (as N)","mg/L",2020,10,0.4,4.4000000000000004,"00618 (Highest result 06/02/20)"]
["Nitrite (as N)","mg/L",2020,1,0.4,"< 0.4","00620"]
["Perchlorate","ppb",2020,6,4,"< 4","A-031"]
["Selenium","ppb",2020,50,5,"< 5","01147"]
["Thallium","ppb",2020,2,1,"< 1","01059"]
["Volatile Organic Chemicals (VOCs)"]
["Benzene","ppb",2020,1,0.5,"< 0.5","34030"]
["Carbon Tetrachloride","ppb",2020,0.5,0.5,"< 0.5","32102"]
["1,2-Dichlorobenzene","ppb",2020,600,0.5,"< 0.5","34536"]
["1,4-Dichlorobenzene","ppb",2020,5,0.5,"< 0.5","34571"]
["1,1-Dichloroethane","ppb",2020,5,0.5,"< 0.5","34496"]
["1,2-Dichloroethane","ppb",2020,0.5,0.5,"< 0.5","34531"]
["1,1-Dichloroethylene","ppb",2020,6,0.5,"< 0.5","34501"]
["cis-1,2-Dichloroethylene","ppb",2020,6,0.5,"< 0.5","77093"]
["trans-1,2-Dichloroethylene","ppb",2020,10,0.5,"< 0.5","34546"]
["Dichloromethane (Methyl Chloride)","ppb",2020,5,0.5,"< 0.5","34423"]
["1,3-Dichloropropene","ppb",2020,0.5,0.5,"< 0.5","34561"]
["1,2-Dichloropropane","ppb",2020,5,0.5,"< 0.5","34541"]
["Ethylbenzene","ppb",2020,300,0.5,"< 0.5","34371"]
["Methyl-tert-butyl ether (MTBE)","ppb",2020,13,3,"< 3","46491"]
["Styrene","ppb",2020,100,0.5,"< 0.5","77128"]
["1,1,2,2-Tetrachloroethane","ppb",2020,1,0.5,"< 0.5","34516"]
["Tetrachloroethylene","ppb",2020,5,0.5,"< 0.5","34475"]
["Toluene","ppb",2020,150,0.5,"< 0.5","34010"]
["1,2,4 Trichlorobenzene","ppb",2020,5,0.5,"< 0.5","34551"]
["1,1,1-Trichloroethane","ppb",2020,200,0.5,"< 0.5","34506"]
["1,1,2-Trichloroethane","ppb",2020,5,0.5,"< 0.5","34511"]
["Trichloroethylene (TCE)","ppb",2020,5,0.5,"< 0.5","39180"]
["Trichlorofluoromethane (Freon-11)","ppb",2020,150,5,"< 5","34488"]
["1,1,2-Trichloro-1,2,2-Trifluoroethane \n(Trichlorotrifluoroethane)","ppb",2020,1200,10,"< 10","81611"]
["Vinyl Chloride","ppb",2020,0.5,0.5,"< 0.5","39175"]
["Xylenes (Total)","ppb",2020,1750,0.5,"< 0.5","81551"]
["Synthetic Organic Chemicals (SOCs)"]
["Alachlor","ppb",2020,2,1,"< 1","77825"]
["Atrazine","ppb",2020,1,0.5,"< 0.5","39033"]
["Bentazon","ppb",2020,18,2,"< 2",38710]
["Benzo (a) pyrene","ppb",2020,0.2,0.1,"< 0.1","34247"]
[]
["Parameter","Units","Year \nTested","MCL","DLR","Chino I\nDesalter","Comments"]
["PRIMARY  STANDARDS - Mandatory Health-Related Standards"]
["Synthetic Organic Chemicals (SOCs) (Continued)"]
["Carbofuran","ppb",2020,18,5,"< 5","81405"]
["2,4-D","ppb",2020,70,10,"< 10","39730"]
["Dalapon","ppb",2020,200,10,"< 10","38432"]
["Di (2-ethylhexyl) adipate","ppb",2020,400,5,"< 5","A -26"]
["Di (2-ethylhexyl) phthalate","ppb",2020,4,3,"< 3","39100"]
["Dibromochloropropane (DBCP)","ppb",2020,0.2,0.01,"< 0.01","38761"]
["Dinoseb","ppb",2020,7,2,"< 2","81287"]
["Diquat","ppb",2020,20,0.4,0,"78885"]
["Endothall","ppb",2020,100,45,"< 45","38926"]
["Endrin","ppb",2020,2,0.1,"< 0.1","39390"]
["Ethylene Dibromide (EDB)","ppb",2020,0.05,0.02,"< 0.02","77651"]
["Glyphosate","ppb",2020,700,25,"< 25","79743"]
["Heptachlor","ppb",2020,0.01,0.01,"< 0.01","39410"]
["Heptachlor Epoxide","ppb",2020,0.01,0.01,"< 0.01","39420"]
["Hexachlorobenzene","ppb",2020,1,0.5,"< 0.5","39700"]
["Hexachlorocyclopentadiene","ppb",2020,50,1,"< 1","34386"]
["Lindane","ppb",2020,0.2,0.2,"< 0.2","39340"]
["Methoxychlor","ppb",2020,30,10,"< 10","39480"]
["Molinate","ppb",2020,20,2,"< 2","82199"]
["Oxamyl (Vydate)","ppb",2020,50,20,"< 20","38865"]
["Pentachlorophenol","ppb",2020,1,0.2,"< 0.2","39032"]
["Picloram","ppb",2020,500,1,"< 1","39720"]
["Polychlorinated Biphenyls (PCBs)\n(as decachlorobiphenyl)","ppb",2020,0.5,0.5,"< 0.5","39516"]
["Simazine","ppb",2020,4,1,"< 1","39055"]
["Thiobencarb","ppb",2020,70,1,"< 1","A - 001"]
["Toxaphene","ppb",2020,3,1,"< 1","39400"]
["2,3,7,8-TCDD (Dioxin)","ppb",2020,30,5,0,"34676"]
["2,4,5-TP (Silvex)","ppb",2020,50,1,"< 1","39045"]
["Microbiological Constituents"]
["Total Coliform Bacteria ","Highest % of Monthly Positives",2020,"(1)","NA",0,"(1) NOTE:  None"]
["Fecal Coliform or E.coli","Highest % of Monthly Positives",2020,"(2)","NA",0,"(2) NOTE:  None"]
["Radiological"]
["Gross Alpha","pCi/L",2020,15,3,0.70499999999999996,1501]
["Disinfectant residuals, disinfection by-products, and disinfection by-products precursors"]
["Chlorine","ppm",2020,"4.0","NA","1.51","(a) Annual average of product water delivered to Chino and JCSD."]
["Chloramine","ppm",2020,"4.0","NA","1.57","(b) Annual average of product water delivered to Chino Hills."]
["Total Trihalomethanes (THM'S/TTHM)","ppb",2020,80,"NA","< 0.5","82080"]
[" - Bromodichloromethane","ppb",2020,"NA",1,"< 1","32101"]
[" - Bromoform","ppb",2020,"NA",1,"< 1","32104"]
[" - Chloroform","ppb",2020,"NA",1,"< 1","32106"]
[" - Dibromochloromethane","ppb",2020,"NA",1,"< 1","32105"]
["Haloacetic Acids (Five) (HAA5)","ppb",2020,60,2,"< 2","A - 049"]
["Parameter","Units","Year \nTested","MCL","DLR","Chino I\nDesalter","Comments"]
["Parameter","Units","Year \nTested","MCL","DLR","Chino I\nDesalter","Comments"]
["PRIMARY  STANDARDS - Mandatory Health-Related Standards"]
["Disinfectant residuals, disinfection by-products, and disinfection by-products precursors (Continued)"]
[" - Monochloroacetic Acid","ppb",2020,"NA",2,"< 2","A - 042"]
[" - Dichloroacetic Acid","ppb",2020,"NA",1,"< 1","77288"]
[" - Trichloroacetic Acid","ppb",2020,"NA",1,"< 1","82723"]
[" - Monobromoacetic Acid","ppb",2020,"NA",1,"< 1","A - 041"]
[" - Dibromoacetic Acid","ppb",2020,"NA",1,"< 1","82721"]
["Total Organic Carbon (TOC)","ppm",2020,"NA",0.3,"< 0.3","00680"]
["SECONDARY  STANDARDS - Aesthetic Standards"]
["Aluminum","ppb",2020,1000,50,"< 50","01105"]
["Color","Color\nUnits",2020,15,"NA","< 3","00081"]
["Chloride","ppm",2020,500,"NA",110,"00940"]
["Copper","ppb",2020,1000,"<50","< 50","01042"]
["Foaming Agents (MBAS)","ppm",2020,0.5,"NA","< 0.08","38260"]
["Iron","ppb",2020,300,100,"< 100","01045"]
["Manganese","ppb",2020,50,20,"< 20","01055"]
["Methyl-tert-butyl ether (MTBE)","ppb",2020,13,3,"< 3",46491]
["Odor - Threshold","TON",2020,3,1,"< 1","00086"]
["Silver","ppb",2020,100,10,"< 10","01077"]
["Specific Conductance","uS/cm",2020,1600,"NA",480,"00095"]
["Sulfate","ppm",2020,500,0.5,1,"00945"]
["Thiobencarb","ppb",2020,70,1,"< 1","A - 001"]
["Total Dissolved Solids (TDS)","ppm",2020,1000,"NA",340,"70300"]
["Turbidity","NTU",2020,5,0.1,0.21,"82079"]
["Zinc","ppb",2020,5000,50,"< 50","01092"]
["OTHER MONITORED PARAMETERS "]
["General Mineral and Physical"]
["Bicarbonate","ppm",2020,"NA","NA",74,"00440"]
["Calcium","ppm",2020,"NA","NA",47,"00916"]
["Carbonate","ppm",2020,"NA","NA","< 5","00445"]
["Hydroxide","ppm",2020,"NA","NA","< 5","71830"]
["Magnesium","ppm",2020,"NA","NA",11,"00927"]
["pH","Std. Units",2020,"NA","NA",7.7,"00403"]
["Potassium","ppm",2020,"NA","NA",1,"00937"]
["Sodium","ppm",2020,"NA","NA",29,"00929"]
["Total Alkalinity","ppm",2020,"NA","NA",74,"00410"]
["Total Hardness","ppm",2020,"NA","NA",160,"00900"]
["Additional Analyses"]
["Total Silica","ppm",2020,"NA","NA",8,"00955"]
["Boron","ppb",2020,"NA",100,"< 100","01020"]
["N-Nitrosodimethylamine (NDMA)","ppb",2020,"NA",4.0000000000000001E-3,"< 0.004","34438 - C0G0635"]
["1,2,3-Trichloropropane (1,2,3-TCP)","ppb",2020,5.0000000000000001E-3,5.0000000000000001E-3,"< 0.005","77443"]
[" "]

{"sheet":"Lab Data","index":1,"n_rows":62,"n_cols":24,"rows_kept":62,"cut":false,"hidden":false,"merged":[[47,0,50,0],[51,0,55,0],[25,0,29,0],[30,0,33,0],[38,0,42,0],[43,0,46,0],[34,0,37,0],[4,0,7,0],[8,0,11,0],[17,0,20,0],[21,0,24,0],[12,0,16,0],[0,20,1,22],[1,2,1,7],[1,8,1,10],[1,11,1,13],[1,14,1,19],[0,2,0,7],[0,8,0,19]]}
[null,null,"Blended Product Water",null,null,null,null,null,"Clearwell Boosters ",null,null,null,null,null,null,null,null,null,null,null,"Product Average"]
[null,null,"Before Clearwell",null,null,null,null,null,"Chino",null,null,"Chino Hills",null,null,"JCSD"]
[2020,null,"NO3","NO3-N","TDS","pH","EC","Langelier","NO3","NO3-N","TDS","NO3","NO3-N","TDS","NO3","NO3-N","TDS","pH","EC","Langelier","Langelier","TCE","123TCP"]
[null,null,"mg/L","mg/L","mg/L",null,"umhos/cm","Index","mg/L","mg/L","mg/L","mg/L","mg/L","mg/L","mg/L","mg/L","mg/L",null,"umhos/cm","Index","Index","ug/L","ug/L"]
["Jan",7,{"$f":"D5*4.4268","v":8.4109199999999991},1.9,390,7.8,520,0.03,{"$f":"J5*4.4268","v":10.18164},2.2999999999999998,370,{"$f":"M5*4.4268","v":10.624319999999999},2.4,370,{"$f":"P5*4.4268","v":10.18164},2.2999999999999998,380,7.9,510,0.12,{"$f":"H5+T5/2","v":0.09}]
[null,14,{"$f":"D6*4.4268","v":7.0828800000000003},1.6,270,7.7,490,-7.0000000000000007E-2,{"$f":"J6*4.4268","v":7.0828800000000003},1.6,310,{"$f":"M6*4.4268","v":6.6402000000000001},1.5,280,{"$f":"P6*4.4268","v":7.0828800000000003},1.6,280,7.7,510,0.13,{"$f":"H6+T6/2","v":-5.0000000000000044E-3},"<0.5","<0.005","C0A1159"]
[null,21,7.0828800000000003,1.6,430,7.6,550,-0.27,7.9682400000000007,1.8,340,7.9682400000000007,1.8,340,7.9682400000000007,1.8,330,7.7,520,0.13,-0.20500000000000002]
[null,28,8.8536000000000001,2,310,7.6,500,-0.02,7.5255599999999996,1.7,310,7.5255599999999996,1.7,330,7.9682400000000007,1.8,320,7.6,520,-0.05,-4.4999999999999998E-2]
["Feb",4,{"$f":"D9*4.4268","v":7.5255599999999996},1.7,360,7.8,520,0.09,{"$f":"J9*4.4268","v":7.0828800000000003},1.6,400,{"$f":"M9*4.4268","v":7.0828800000000003},1.6,400,{"$f":"P9*4.4268","v":7.0828800000000003},1.6,400,7.8,520,0.06,0.12]
[null,11,9.7389600000000005,2.2000000000000002,360,7.5,500,0.36,13.2804,3,280,13.2804,3,280,13.2804,3,280,7.4,400,-0.52,9.9999999999999978E-2,"<0.5","<0.005","C0B1266"]
[null,18,16.821839999999998,3.8,180,7.7,310,-0.3,10.624319999999999,2.4,290,11.067,2.5,280,11.509680000000001,2.6,300,7.7,470,0,-0.3]
[null,25,7.0828800000000003,1.6,290,7.5,450,-0.15,8.8536000000000001,2,280,8.8536000000000001,2,290,9.2962800000000012,2.1,290,7.5,430,-0.4,-0.35]
["Mar",3,{"$f":"D13*4.4268","v":8.8536000000000001},2,410,7.5,530,-0.48,{"$f":"J13*4.4268","v":8.8536000000000001},2,340,{"$f":"M13*4.4268","v":8.8536000000000001},2,350,{"$f":"P13*4.4268","v":8.8536000000000001},2,340,7.6,null,-0.14000000000000001,-0.55000000000000004]
[null,9,{"$f":"D14*4.4268","v":8.4109199999999991},1.9,440,7.6,580,-0.23,{"$f":"J14*4.4268","v":10.18164},2.2999999999999998,340,{"$f":"M14*4.4268","v":9.2962800000000012},2.1,340,{"$f":"P14*4.4268","v":8.8536000000000001},2,340,7.7,540,0.17,-0.14500000000000002,"<0.5","<0.005","C0C1161"]
[null,17,9.7389600000000005,2.2000000000000002,350,7.7,500,-0.01,9.7389600000000005,2.2000000000000002,330,9.7389600000000005,2.2000000000000002,300,9.7389600000000005,2.2000000000000002,320,7.7,480,-0.03,-2.5000000000000001E-2]
[null,24,10.18164,2.2999999999999998,350,7.7,520,-0.02,9.2962800000000012,2.1,440,9.2962800000000012,2.1,450,9.7389600000000005,2.2000000000000002,420,7.6,580,-0.13,-8.5000000000000006E-2]
[null,31,{"$f":"D17*4.4268","v":10.18164},2.2999999999999998,420,7.7,590,0.11,{"$f":"J17*4.4268","v":14.60844},3.3,380,{"$f":"M17*4.4268","v":15.936480000000001},3.6,400,{"$f":"P17*4.4268","v":14.165760000000001},3.2,410,7.6,590,0.11,0.16500000000000001]
["Apr",7,13.723080000000001,3.1,370,7.7,560,0.12,11.509680000000001,2.6,400,11.067,2.5,370,11.509680000000001,2.6,400,7.7,570,0.08,0.16]
[null,14,19.035239999999998,4.3,340,7.8,580,0.28999999999999998,12.39504,2.8,260,11.509680000000001,2.6,260,14.60844,3.3,320,7.8,580,0.25,0.41499999999999998,"<0.5","<0.005","COD1818"]
[null,21,11.067,2.5,320,7.6,460,-0.18,11.067,2.5,350,11.067,2.5,380,11.067,2.5,360,7.6,520,0.01,-0.17499999999999999]
[null,28,14.60844,3.3,310,7.4,500,-0.1,15.051119999999999,3.4,330,15.051119999999999,3.4,370,15.051119999999999,3.4,350,7.4,490,-0.35,-0.27500000000000002]
["May",5,{"$f":"D22*4.4268","v":15.936480000000001},3.6,330,7.7,560,0.02,15.4938,3.5,310,15.936480000000001,3.6,320,15.4938,3.5,310,7.6,550,-7.0000000000000007E-2,-1.5000000000000003E-2]
[null,11,15.051119999999999,3.4,360,7.8,550,0.17,16.379160000000002,3.7,380,16.821839999999998,3.8,370,16.379160000000002,3.7,360,7.8,550,0.14000000000000001,0.24000000000000002,"<0.5","<0.005","C0E1191"]
[null,19,13.723080000000001,3.1,380,7.7,540,-0.06,15.051119999999999,3.4,420,15.051119999999999,3.4,380,15.051119999999999,3.4,350,7.7,550,0.04,-3.9999999999999994E-2]
[null,26,13.2804,3,440,7.8,560,0.03,16.379160000000002,3.7,440,17.264520000000001,3.9,340,16.379160000000002,3.7,390,7.8,550,0.19,0.125]
["June",2,18.592560000000002,4.2,250,7.7,420,-2.9000000000000001E-2,19.477920000000001,4.4000000000000004,240,19.9206,4.5,260,19.477920000000001,4.4000000000000004,250,7.5,430,-0.54,-0.29900000000000004]
[null,9,16.821839999999998,3.8,380,7.8,480,0.03,16.379160000000002,3.7,350,16.379160000000002,3.7,380,16.379160000000002,3.7,520,7.7,510,0.08,7.0000000000000007E-2,"<0.5","<0.005","C0F1235"]
[null,16,19.035239999999998,4.3,310,7.8,460,-7.0000000000000007E-2,16.821839999999998,3.8,400,16.379160000000002,3.7,390,16.821839999999998,3.8,400,7.9,460,0.23,4.4999999999999998E-2]
[null,23,18.592560000000002,4.2,330,7,520,-0.63,16.379160000000002,3.7,360,16.821839999999998,3.8,360,16.821839999999998,3.8,360,7,510,-0.69,-0.97499999999999998]
[null,30,14.165760000000001,3.2,320,8,510,0.4,13.723080000000001,3.1,320,14.165760000000001,3.2,340,13.723080000000001,3.1,310,8,500,0.32,0.56000000000000005]
["July",6,14.60844,3.3,300,8,510,0.18,18.592560000000002,4.2,270,18.592560000000002,4.2,280,15.4938,3.5,360,7.9,510,0.09,0.22499999999999998,"<0.5","<0.005","C0G0629"]
[null,14,20.36328,4.5999999999999996,390,7.7,500,-0.06,18.592560000000002,4.2,360,16.821839999999998,3.8,330,16.379160000000002,3.7,390,7.8,480,-0.09,-0.105]
[null,21,17.264520000000001,3.9,450,7.8,600,7.0000000000000007E-2,18.592560000000002,4.2,390,18.592560000000002,4.2,400,18.592560000000002,4.2,410,7.8,550,0.17,0.15500000000000003]
[null,28,15.051119999999999,3.4,330,8,520,0.48,16.821839999999998,3.8,390,16.379160000000002,3.7,430,16.821839999999998,3.8,360,8,550,0.39,0.67500000000000004]
["Aug",4,15.051119999999999,3.4,270,7.9,520,0.39,15.4938,3.5,280,14.60844,3.3,340,15.4938,3.5,280,7.8,530,0.24,0.51]
[null,11,16.379160000000002,3.7,360,7.9,480,0.2,16.379160000000002,3.7,390,16.379160000000002,3.7,360,16.379160000000002,3.7,330,7.9,490,0.22,0.31,"<0.5","<0.005","C0H1432"]
[null,18,17.7072,4,310,8,540,0.41,15.936480000000001,3.6,350,15.936480000000001,3.6,340,15.936480000000001,3.6,380,7.9,560,0.35,0.58499999999999996]
[null,25,16.379160000000002,3.7,390,8,560,0.51,15.051119999999999,3.4,380,15.936480000000001,3.6,370,15.936480000000001,3.6,390,7.6,450,0.26,0.64]
["Sept",1,12.39504,2.8,360,7.8,570,0.14000000000000001,16.379160000000002,3.7,330,16.821839999999998,3.8,330,16.379160000000002,3.7,360,7.8,540,0.19,0.23500000000000001]
[null,8,15.4938,3.5,490,7.6,580,-0.23,15.4938,3.5,340,15.4938,3.5,320,15.936480000000001,3.6,340,7.7,530,0.08,-0.19,"<0.5","<0.005","C0I0955"]
[null,15,14.60844,3.3,300,7.7,480,-0.01,12.39504,2.8,300,12.39504,2.8,310,12.39504,2.8,300,7.7,490,-0.02,-0.02]
[null,22,14.165760000000001,3.2,330,7.6,500,-0.19,13.723080000000001,3.1,290,13.2804,3,350,13.723080000000001,3.1,310,7.7,490,-0.05,-0.215]
[null,29,16.379160000000002,3.7,320,7.7,510,-0.01,15.936480000000001,3.6,310,15.936480000000001,3.6,310,15.051119999999999,3.4,320,7.7,510,0.04,0.01]
["Oct",6,17.7072,4,260,7.7,530,-0.06,16.379160000000002,3.7,320,15.051119999999999,3.4,300,15.4938,3.5,330,7.6,550,-0.04,-0.08]
[null,13,8.8536000000000001,2,510,7.6,590,-0.14000000000000001,10.624319999999999,2.4,550,10.624319999999999,2.4,500,10.624319999999999,2.4,520,7.8,600,0.16,-6.0000000000000012E-2,"<0.5","<0.005","C0J1638"]
[null,20,8.8536000000000001,2,330,7.8,540,0.23,8.8536000000000001,2,290,9.2962800000000012,2.1,330,9.2962800000000012,2.1,300,7.8,550,0.16,0.31]
[null,27,13.2804,3,320,7.9,540,0.3,12.837719999999999,2.9,340,12.837719999999999,2.9,370,12.837719999999999,2.9,320,7.8,550,0.2,0.4]
["Nov",3,11.952360000000001,2.7,350,7.6,570,0.04,10.624319999999999,2.4,360,10.624319999999999,2.4,360,11.067,2.5,350,7.8,590,0.25,0.16500000000000001]
[null,10,9.7389600000000005,2.2000000000000002,270,7.9,560,0.36,9.2962800000000012,2.1,300,9.2962800000000012,2.1,360,9.2962800000000012,2.1,300,7.8,540,0.12,0.42,"<0.5","<0.005","C0K1357"]
[null,17,14.165760000000001,3.2,390,7.7,670,0,11.952360000000001,2.7,270,11.952360000000001,2.7,310,12.39504,2.8,290,7.7,530,0.08,0.04]
[null,24,13.723080000000001,3.1,280,7.5,520,-0.26,12.39504,2.8,280,12.39504,2.8,290,12.39504,2.8,280,7.6,540,-0.15,-0.33500000000000002]
["Dec",1,15.4938,3.5,320,7.3,540,-0.55000000000000004,12.837719999999999,2.9,340,11.509680000000001,2.6,320,13.2804,3,330,7.7,580,-0.02,-0.56000000000000005]
[null,8,7.0828800000000003,1.6,440,7.7,610,0.13,7.0828800000000003,1.6,440,7.0828800000000003,1.6,420,7.0828800000000003,1.6,440,7.5,600,-0.09,8.5000000000000006E-2,"<0.5","<0.005","C0L1048"]
[null,15,15.051119999999999,3.4,300,7.8,570,0.18,13.2804,3,300,12.39504,2.8,300,13.723080000000001,3.1,290,7.5,480,-0.31,2.4999999999999994E-2]
[null,22,10.18164,2.2999999999999998,380,7.7,560,0,10.624319999999999,2.4,370,10.624319999999999,2.4,400,10.624319999999999,2.4,360,7.7,570,0.05,2.5000000000000001E-2]
[null,29,15.051119999999999,3.4,330,8,540,0.44,14.60844,3.3,340,14.165760000000001,3.2,340,14.60844,3.3,350,7.8,550,0.17,0.52500000000000002]
[]
[]
[]
["Min.",null,{"$f":"MIN(C5:C56)","v":7.0828800000000003},1.6,180,7,310,-0.63,7.0828800000000003,1.6,240,6.6402000000000001,1.5,260,7.0828800000000003,1.6,250,7,400,-0.69,-1.5,"<0.50","<0.005"]
["Avg.",null,{"$f":"AVERAGE(C5:C56)","v":13.280399999999998},3,347.69230769230768,7.713461538461539,528.26923076923072,3.0403846153846163E-2,13.118651538461542,2.963461538461539,343.26923076923077,13.050546923076924,2.9480769230769228,346.15384615384613,13.110138461538465,2.9615384615384617,347.69230769230768,7.700000000000002,524.50980392156862,3.0576923076923074E-2,-0.5,"<0.50","<0.005"]
["Max.",null,{"$f":"MAX(C5:C56)","v":20.36328},4.5999999999999996,510,8,670,0.51,19.477920000000001,4.4000000000000004,550,19.9206,4.5,500,19.477920000000001,4.4000000000000004,520,8,600,0.39,0.2,"<0.50","<0.005"]